    Synthesis and Ngdbuild  Report
    synthesis:  version Diamond_1.2_Production (79)
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved. Copyright (c) 1995 AT&T Corp.   All rights reserved. Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved. Copyright (c) 2001 Agere Systems   All rights reserved. Copyright (c) 2002-2011 Lattice Semiconductor Corporation,  All rights reserved.
    Sun Feb 27 23:02:53 2011

    Command Line:  synthesis -f control_SoC_demo_impl1_lattice.synproj

    -- all messages logged in file synthesis.log

    Synthesis Options

    INFO: Synthesis Options: (LSE-1021)
    INFO: -a option is = MachXO2
    INFO: -s option is = 3
    INFO: -t option is = CSBGA132
    INFO: -d option is = LCMXO2-1200ZE
    INFO: Using package CSBGA132
    INFO: Using speed grade 3
    INFO:
    INFO: ##########################################################
    INFO: ### Lattice Family : MachXO2
    INFO: ### Device  : LCMXO2-1200ZE
    INFO: ### Package : CSBGA132
    INFO: ### Speed   : 3
    INFO: ##########################################################
    INFO:
    INFO: Optimization Goal = Balanced
    INFO: Top level module name = control_soc_demo
    INFO: Target Frequency = 200.000000 MHz
    INFO: Max Fanout = 1000
    INFO: Timing Path count = 3
    INFO: bram Utilization = 100.000000 %
    INFO: dsp usage = TRUE (default)
    INFO: dsp utilization = 100 (default)
    INFO: fsm_encoding_style = auto
    INFO: Mux style = Auto
    INFO: Use Carry Chain = TRUE
    INFO: carry_chain_length = 0
    INFO: Use IO Insertion = TRUE
    INFO: Use IO Reg = TRUE
    INFO: Resource Sharing = TRUE
    INFO: Propagate Constants = TRUE
    INFO: Remove Duplicate Registers = TRUE
    INFO: force_gsr = auto
    INFO: ROM style = auto
    INFO: RAM style = auto
    INFO: -p C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project (searchpath added)
    INFO: -p C:/Diamond/diamond/1.2/ispfpga/xo2c00/data (searchpath added)
    INFO: -p C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/impl1 (searchpath added)
    INFO: -p C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project (searchpath added)
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/audio_buffer.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/clk_gen.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/wave_read.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/pwm.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/LCDEncoding4to1.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/lcdencoding4to1com.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/uptime_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1046/source/i2c_master_registers.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1046/source/i2c_master_bit_ctrl.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1046/source/i2c_master_byte_ctrl.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1046/source/i2c_master_wb_top.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1044/Source/Spi_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../latticemico8_v3_1_verilog/source/isp8_core.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/rom_ebr_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/IPexpress/PLL.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/pll_soft_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1066/source/verilog/box_ave.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1066/source/verilog/sigmadelta_adc.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1066/source/verilog/adc_top.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/adc_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1042/source/modem.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1042/source/uart_core.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/lm8_top.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../latticemico8_v3_1_verilog/source/isp8_io_cntl.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../latticemico8_v3_1_verilog/source/isp8_flow_cntl.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../latticemico8_v3_1_verilog/source/isp8_alu.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../latticemico8_v3_1_verilog/source/isp8_idec.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../rd1043/source/lm8_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/led_sw_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/reset_gen.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/clk_switch.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/clksource_wb.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/debounce.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/lcd4digit.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/source/PowerCntr.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/control_soc_demo.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/ringosc.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/oscclkclean.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/source/IPexpress/EFB_Module.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/source/IPexpress/BankController.v
    INFO: Verilog design file = C:/Documents and Settings/cwest/Desktop/MachXO2_Pico_Demos/SoC/Demo_MachXO2_Pico_SoC15_Diamond_Golden_2MHz_BCntr_cap/Demo_MachXO2_Control_SoC/project/../source/capsense.v
    INFO: Ngd file = control_SoC_demo_impl1.ngd
    INFO: -sdc option: sdc file input not used
    INFO: -lpf option: output file option is OFF
    INFO: hardtimer checking is enabled (default); -dt option not used
    INFO: -r option is OFF [ Remove LOC Properties is OFF ]
    -- Technology family check...
    INFO: The default vhdl library search path is now "c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/impl1" (VHDL-1504)

    Compile Design

    INFO: Compile Design Begin
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/control_soc_demo.v(45): INFO: compiling module control_soc_demo (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/source/ipexpress/bankcontroller.v(8): INFO: compiling module BankController (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/reset_gen.v(46): INFO: compiling module reset_gen (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/led_sw_wb.v(46): INFO: compiling module lcd_sw_wb (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/clksource_wb.v(46): INFO: compiling module clkselect_wb (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/ringosc.v(46): INFO: compiling module RingOSC (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/oscclkclean.v(46): INFO: compiling module oscclkclean (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/clk_switch.v(1): INFO: compiling module clk_switch (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1043/source/lm8_wb.v(47): INFO: compiling module lm8_wb(LM8_ADDR_W=24,NUM_DECODE=4) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/lm8_top.v(46): INFO: compiling module isp8(FAMILY_NAME="XO2",PROM_FILE="prom_init.hex",PORT_AW=8,EXT_AW=24,PROM_AW=11,PROM_AD=2048,REGISTERS_16=0,PGM_STACK_AW=4,PGM_STACK_AD=16) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_core.v(42): INFO: compiling module isp8_core(FAMILY_NAME="XO2",PROM_FILE="prom_init.hex",PORT_AW=8,EXT_AW=24,PROM_AW=11,PROM_AD=2048,REGISTERS_16=0,PGM_STACK_AW=4,PGM_STACK_AD=16) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_idec.v(40): INFO: compiling module isp8_idec(PROM_AW=11) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_alu.v(41): INFO: compiling module isp8_alu(FAMILY_NAME="XO2") (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_alu.v(135): INFO: compiling module pmi_addsub(pmi_data_width=8,pmi_result_width=8,pmi_sign="off",pmi_family="XO2",module_type="pmi_addsub") (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_flow_cntl.v(41): INFO: compiling module isp8_flow_cntl(PGM_STACK_AW=4,PGM_STACK_AD=16,PROM_AW=11,FAMILY_NAME="XO2") (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/lm8_top.v(142): INFO: compiling module pmi_distributed_spram(pmi_addr_depth=16,pmi_addr_width=4,pmi_data_width=13,pmi_regmode="noreg",pmi_init_file="none",pmi_init_file_format="binary",pmi_family="XO2",module_type="pmi_distributed_spram") (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_io_cntl.v(39): INFO: compiling module isp8_io_cntl(PORT_AW=8) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_core.v(513): INFO: compiling module pmi_rom_renamed_due_excessive_length_1 (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_core.v(488): INFO: compiling module pmi_distributed_dpram(pmi_addr_depth=32,pmi_addr_width=5,pmi_data_width=8,pmi_regmode="noreg",pmi_init_file="none",pmi_init_file_format="binary",pmi_family="XO2",module_type="pmi_distributed_dpram") (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/lm8_top.v(142): INFO: compiling module pmi_distributed_spram(pmi_addr_depth=32,pmi_addr_width=5,pmi_data_width=8,pmi_regmode="noreg",pmi_init_file="none",pmi_init_file_format="binary",pmi_family="XO2",module_type="pmi_distributed_spram") (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1042/source/uart_core.v(52): INFO: compiling module uart_core(CLK_IN_MHZ=2,BAUD_RATE=115200,ADDRWIDTH=3,DATAWIDTH=8,FIFO=0) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1042/source/intface.v(51): INFO: compiling module intface(CLK_IN_MHZ=2,BAUD_RATE=115200,ADDRWIDTH=3,DATAWIDTH=8,FIFO=0) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1042/source/rxcver.v(49): INFO: compiling module rxcver(DATAWIDTH=8,FIFO=0) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1042/source/txmitt.v(48): INFO: compiling module txmitt(DATAWIDTH=8,FIFO=0) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1042/source/modem.v(49): INFO: compiling module modem(DATAWIDTH=8) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/adc_wb.v(46): INFO: compiling module adc_wb (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1066/source/verilog/adc_top.v(62): INFO: compiling module ADC_top (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1066/source/verilog/sigmadelta_adc.v(62): INFO: compiling module sigmadelta_adc(ADC_WIDTH=8,ACCUM_BITS=10,LPF_DEPTH_BITS=3) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1066/source/verilog/box_ave.v(66): INFO: compiling module box_ave(ADC_WIDTH=8,LPF_DEPTH_BITS=3) (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/rom_ebr_wb.v(45): INFO: compiling module rom_ebr_wb (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_core.v(513): INFO: compiling module pmi_rom_renamed_due_excessive_length_2 (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/source/ipexpress/efb_module.v(8): INFO: compiling module EFB_Module (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/capsense.v(62): INFO: compiling module capsense (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/lcd4digit.v(1): INFO: compiling module LCD4Digit (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/lcdencoding4to1com.v(2): INFO: compiling module LCDEncoding4to1com (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/pwm.v(2): INFO: compiling module PWM (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/lcdencoding4to1.v(2): INFO: compiling module LCDEncoding4to1 (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/debounce.v(1): INFO: compiling module PushButton_Debouncer (VERI-1018)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/source/powercntr.v(8): INFO: compiling module PowerCntr (VERI-1018)
    INFO: ######## Missing driver on net : wb_ack[15], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_ack[11], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_ack[10], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_ack[3], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[127], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[126], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[125], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[124], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[123], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[122], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[121], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[120], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[95], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[94], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[93], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[92], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[91], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[90], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[89], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[88], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[87], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[86], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[85], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[84], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[83], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[82], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[81], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[80], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[31], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[30], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[29], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[28], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[27], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[26], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[25], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : wb_dat_i[24], patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : rstn, patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : \UART_INST/RI_N, patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : \UART_INST/DSR_N, patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : \UART_INST/CTS_N, patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : \UART_INST/DCD_N, patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : \PowerCntr_inst/CFGSTDBY, patching with GND... (LSE-1017)
    INFO: ######## Missing driver on net : \PowerCntr_inst/CFGWAKE, patching with GND... (LSE-1017)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_flow_cntl.v(229): WARNING: Register \lm8_inst/u1_isp8/u1_isp8_flow_cntl/intr_reg0 is stuck at Zero (VDB-5013)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../latticemico8_v3_1_verilog/source/isp8_flow_cntl.v(375): WARNING: Register \lm8_inst/u1_isp8/u1_isp8_flow_cntl/intr_ack_int is stuck at Zero (VDB-5013)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/control_soc_demo.v(664): WARNING: Register OscReg1 is stuck at Zero (VDB-5013)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/capsense.v(153): WARNING: Bit 0 of Register \capsense_inst/FastCounter2 is stuck at Zero (VDB-5010)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/capsense.v(230): WARNING: Bit 0 of Register \capsense_inst/SampleCounter is stuck at Zero (VDB-5010)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/capsense.v(230): WARNING: Register \capsense_inst/touched1 is stuck at Zero (VDB-5013)
    WARNING: Bit 0 of Register \UART_INST/u_rxcver/cs_state_FSM is stuck at Zero (VDB-5010)
    WARNING: Bit 1 of Register \UART_INST/u_rxcver/cs_state_FSM is stuck at Zero (VDB-5010)
    WARNING: Bit 2 of Register \UART_INST/u_rxcver/cs_state_FSM is stuck at Zero (VDB-5010)
    WARNING: Bit 0 of Register \UART_INST/u_intface/cs_state_FSM is stuck at Zero (VDB-5010)
    WARNING: Bit 1 of Register \UART_INST/u_intface/cs_state_FSM is stuck at Zero (VDB-5010)
    WARNING: Bit 2 of Register \UART_INST/u_intface/cs_state_FSM is stuck at Zero (VDB-5010)
    WARNING: Bit 0 of Register \UART_INST/u_txmitt/tx_state_FSM is stuck at Zero (VDB-5010)
    INFO: ######## Converting i/o port : cap_btn1 to OUTPUT ... (LSE-1066)
    INFO: ######## Converting i/o port : cap_btn2 to OUTPUT ... (LSE-1066)
    INFO: ######## Converting i/o port : cap_btn3 to OUTPUT ... (LSE-1066)
    INFO: ######## Converting i/o port : cap_btn4 to OUTPUT ... (LSE-1066)
    WARNING: Skipping pad insertion on scl due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on sda due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on spi_sclk due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on spi_mosi due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on spi_miso due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on Icc_analog_cmp_n due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on Icc_analog_cmp_p due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on Icco_analog_cmp_n due to black_box_pad_pin attribute (LSE-1153)
    WARNING: Skipping pad insertion on Icco_analog_cmp_p due to black_box_pad_pin attribute (LSE-1153)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1042/source/modem.v(124): WARNING: Register dffrs_301_i3 is stuck at Zero (VDB-5013)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../rd1042/source/intface.v(227): WARNING: Register \UART_INST/u_intface/divisor_i15 is stuck at Zero (VDB-5013)
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/oscclkclean.v(123): WARNING: Register \clkselect_wb_inst/oscclkclean_inst/RingOSCmax_i9 is stuck at Zero (VDB-5013)
    INFO: Combinational loop found : 1
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[10]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i11
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[10]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 2
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[9]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i10
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[9]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 3
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[8]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i9
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[8]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 4
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[7]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i8
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[7]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 5
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[6]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i7
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[6]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 6
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[5]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i6
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[5]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 7
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[4]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i5
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[4]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 8
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[3]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i4
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[3]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 9
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[2]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i3
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[2]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 10
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i2
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[1]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 11
    INFO: 	Net \lm8_inst/u1_isp8/prom_addr[0]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/mux_98_i1
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/dout_stack[0]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/pmi_distributed_sprampmi_distributed_spramXO2binarynonenoreg13416
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_flow_cntl/din_stack_w_cz[12]
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_flow_cntl/i107
    INFO: 	Net \lm8_inst/u1_isp8/clrc
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i58
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/instr_l7_0
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i33
    INFO: 	Net \lm8_inst/u1_isp8/u1_isp8_idec/n31
    INFO: 	Instance \lm8_inst/u1_isp8/u1_isp8_idec/i31
    INFO: 	Net \lm8_inst/u1_isp8/instr[1]
    INFO: 	Instance \lm8_inst/u1_isp8/pmi_rompmi_romXO2hexprom_init.hexasyncdisablenoreg18112048
    INFO: Combinational loop found : 12
    INFO: 	Net \clkselect_wb_inst/RingOSCraw
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i7
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/RingOSCb[6]
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/RingOSCb[6]_keep_buf
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/n14
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i12
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/RingOSCb[5]
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/RingOSCb[5]_keep_buf
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/n15
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i11
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/RingOSCb[4]
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/RingOSCb[4]_keep_buf
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/n16
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i10
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/RingOSCb[3]
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/RingOSCb[3]_keep_buf
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/n17
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i9
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/RingOSCb[2]
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/RingOSCb[2]_keep_buf
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/n18
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i8
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/RingOSCb[1]
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/RingOSCb[1]_keep_buf
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/n19
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i6
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/n5
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/i5
    INFO: 	Net \clkselect_wb_inst/RingOSC_inst/RingOSCb[0]
    INFO: 	Instance \clkselect_wb_inst/RingOSC_inst/RingOSCb[0]_keep_buf
    INFO: Combinational loop found : 13
    INFO: 	Net DebounceRingOSCb[0]
    INFO: 	Instance DebounceRingOSCb[0]_keep_buf
    INFO: 	Net n906
    INFO: 	Instance i174
    INFO: 	Net DebounceRingOSCb[16]
    INFO: 	Instance DebounceRingOSCb[16]_keep_buf
    INFO: 	Net n890
    INFO: 	Instance i189
    INFO: 	Net DebounceRingOSCb[15]
    INFO: 	Instance DebounceRingOSCb[15]_keep_buf
    INFO: 	Net n891
    INFO: 	Instance i188
    INFO: 	Net DebounceRingOSCb[14]
    INFO: 	Instance DebounceRingOSCb[14]_keep_buf
    INFO: 	Net n892
    INFO: 	Instance i187
    INFO: 	Net DebounceRingOSCb[13]
    INFO: 	Instance DebounceRingOSCb[13]_keep_buf
    INFO: 	Net n893
    INFO: 	Instance i186
    INFO: 	Net DebounceRingOSCb[12]
    INFO: 	Instance DebounceRingOSCb[12]_keep_buf
    INFO: 	Net n894
    INFO: 	Instance i185
    INFO: 	Net DebounceRingOSCb[11]
    INFO: 	Instance DebounceRingOSCb[11]_keep_buf
    INFO: 	Net n895
    INFO: 	Instance i184
    INFO: 	Net DebounceRingOSCb[10]
    INFO: 	Instance DebounceRingOSCb[10]_keep_buf
    INFO: 	Net n896
    INFO: 	Instance i183
    INFO: 	Net DebounceRingOSCb[9]
    INFO: 	Instance DebounceRingOSCb[9]_keep_buf
    INFO: 	Net n897
    INFO: 	Instance i182
    INFO: 	Net DebounceRingOSCb[8]
    INFO: 	Instance DebounceRingOSCb[8]_keep_buf
    INFO: 	Net n898
    INFO: 	Instance i181
    INFO: 	Net DebounceRingOSCb[7]
    INFO: 	Instance DebounceRingOSCb[7]_keep_buf
    INFO: 	Net n899
    INFO: 	Instance i180
    INFO: 	Net DebounceRingOSCb[6]
    INFO: 	Instance DebounceRingOSCb[6]_keep_buf
    INFO: 	Net n900
    INFO: 	Instance i179
    INFO: 	Net DebounceRingOSCb[5]
    INFO: 	Instance DebounceRingOSCb[5]_keep_buf
    INFO: 	Net n901
    INFO: 	Instance i178
    INFO: 	Net DebounceRingOSCb[4]
    INFO: 	Instance DebounceRingOSCb[4]_keep_buf
    INFO: 	Net n902
    INFO: 	Instance i177
    INFO: 	Net DebounceRingOSCb[3]
    INFO: 	Instance DebounceRingOSCb[3]_keep_buf
    INFO: 	Net n903
    INFO: 	Instance i176
    INFO: 	Net DebounceRingOSCb[2]
    INFO: 	Instance DebounceRingOSCb[2]_keep_buf
    INFO: 	Net n904
    INFO: 	Instance i175
    INFO: 	Net DebounceRingOSCb[1]
    INFO: 	Instance DebounceRingOSCb[1]_keep_buf
    INFO: 	Net n905
    INFO: 	Instance i173
    INFO: 	Net n527
    INFO: 	Instance i172
    c:/documents and settings/cwest/desktop/machxo2_pico_demos/soc/demo_machxo2_pico_soc15_diamond_golden_2mhz_bcntr_cap/demo_machxo2_control_soc/project/../source/pwm.v(76): WARNING: Register \LCD4Digit_inst/LCD_8_inst/state_i2 is stuck at Zero (VDB-5013)
    INFO: GSR inferred on net: n6457 (LSE-1146)
    INFO: Duplicate Register/Latch removal : dffrs_301_i2 is one to one match with dffrs_301_i1
    INFO: Duplicate Register/Latch removal : dffrs_301_i4 is one to one match with dffrs_301_i2
    WARNING: Init file "menu.hex" not found in current directory, will try search paths listed with -p option... (LSE-1089)
    WARNING: Init file "prom_init.hex" not found in current directory, will try search paths listed with -p option... (LSE-1089)
    WARNING: No lpf file will be written because there is no user sdc file
    INFO: Applying 200.000000 MHz constraint to all clocks (LSE-5000)
    INFO: Results of ngd drc checks are available in control_soc_demo_drc.log
    INFO: All blocks are expanded and NGD expansion is successful
    INFO: Writing ngd file control_SoC_demo_impl1.ngd

    Area Report

    INFO: ################### Begin Area Report (control_soc_demo)######################
    INFO: Number of register bits => 598 of 5435 (11 % ) (LSE-1070)
    INFO: AND2 => 10
    INFO: BB => 5
    INFO: BCINRD => 1
    INFO: CCU2D => 93
    INFO: EFB => 1
    INFO: FD1P3AX => 78
    INFO: FD1P3AY => 1
    INFO: FD1P3BX => 14
    INFO: FD1P3DX => 131
    INFO: FD1P3IX => 48
    INFO: FD1S1A => 12
    INFO: FD1S3AX => 173
    INFO: FD1S3AY => 14
    INFO: FD1S3BX => 10
    INFO: FD1S3DX => 80
    INFO: FD1S3IX => 36
    INFO: GSR => 1
    INFO: IB => 4
    INFO: IFS1P3DX => 1
    INFO: ILVDS => 2
    INFO: INV => 45
    INFO: L6MUX21 => 8
    INFO: LUT4 => 670
    INFO: MUX21 => 4
    INFO: OB => 1
    INFO: OBZ => 22
    INFO: OR2 => 7
    INFO: OSCH => 1
    INFO: PCNTR => 1
    INFO: PFUMX => 67
    INFO: XOR2 => 1
    INFO: pmi_addsubXo88 => 1
    INFO: pmi_distributed_dpramXbnonen8532 => 2
    INFO: pmi_distributed_spramXbnonen13416 => 1
    INFO: pmi_distributed_spramXbnonen8532 => 1
    INFO: pmi_romXhmenusdn8101024 => 1
    INFO: pmi_romXhprom_initadn18112048 => 1
    INFO: ################### End Area Report ################## (LSE-1069)

    Clock Report

    INFO: ################### Begin Clock Report ###################### (LSE-1072)
    INFO: Clock Nets
    INFO: Number of Clocks: 11 (LSE-1074)
    INFO:   Net : clk, loads : 392
    INFO:   Net : lcdcounter_12, loads : 96
    INFO:   Net : RingOSCb_0, loads : 35
    INFO:   Net : DebounceRingOSCb_0, loads : 31
    INFO:   Net : lcdcounter_3, loads : 24
    INFO:   Net : VCC_net, loads : 12
    INFO:   Net : oscclk, loads : 9
    INFO:   Net : RingOSCclk, loads : 5
    INFO:   Net : n521, loads : 1
    INFO:   Net : clk_USB_c, loads : 1
    INFO:   Net : ButtonPushed, loads : 1
    INFO: Clock Enable Nets
    INFO: Number of Clock Enables: 61
    INFO: Highest fanout non-clock nets
    INFO: Top 10 highest fanout non-clock nets: (LSE-1076)
    INFO:   Net : wb_rst, loads : 174
    INFO:   Net : n15435, loads : 67
    INFO:   Net : instr_0, loads : 37
    INFO:   Net : addr_20, loads : 30
    INFO:   Net : instr_15, loads : 30
    INFO:   Net : wb_addr_1, loads : 28
    INFO:   Net : instr_13, loads : 28
    INFO:   Net : addr_22, loads : 27
    INFO:   Net : wb_addr_0, loads : 27
    INFO:   Net : instr_14, loads : 27
    INFO: ################### End Clock Report ################## (LSE-1073)

    Timing Report Summary
    --------------
    --------------------------------------------------------------------------------
    Constraint                              |   Constraint|       Actual|Levels
    --------------------------------------------------------------------------------
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk9 [get_nets DebounceRingOSCb[16]]    |  200.000 MHz|   63.784 MHz|     6 *
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk8 [get_nets lcdcounter[3]]           |  200.000 MHz|  156.568 MHz|     2 *
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk7 [get_nets clk_USB_c]               |            -|            -|     0
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk6 [get_nets                          |             |             |
    \clkselect_wb_inst/RingOSC_inst/RingOSCb|             |             |
    [6]]                                    |  200.000 MHz|   77.250 MHz|     8 *
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk5 [get_nets ButtonPushed]            |  200.000 MHz|  267.666 MHz|     1
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk4 [get_nets                          |             |             |
    \clkselect_wb_inst/oscclk]              |  200.000 MHz|  162.681 MHz|     2 *
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk3 [get_nets lcdcounter[12]]          |  200.000 MHz|  280.269 MHz|     1
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk2 [get_nets                          |             |             |
    \clkselect_wb_inst/RingOSCclk]          |  200.000 MHz|  194.666 MHz|     2 *
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk1 [get_nets VCC_net]                 |            -|            -|     0
                                            |             |             |
    create_clock -period 5.000000 -name     |             |             |
    clk0 [get_nets clk]                     |  200.000 MHz|   31.745 MHz|    24 *
                                            |             |             |
    --------------------------------------------------------------------------------

    6 constraints not met.

    Peak Memory Usage: 57 MB

    --------------------------------------------------------------
    Elapsed CPU time for LSE flow : 7.218750 secs
    --------------------------------------------------------------