         Lattice Mapping Report File for Design Module 'Environment_Scanning'

    Design Information

    Command line:   map -a MachXO2 -p LCMXO2-1200ZE -t CSBGA132 -s 3 -oc Commercial
         Environment_Scanning_impl1.ngd -o Environment_Scanning_impl1_map.ncd -pr
         Environment_Scanning_impl1.prf -mp Environment_Scanning_impl1.mrp
         C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_Enviro
         nment_Scanning/project/Environment_Scanning.lpf -c 0
    Target Vendor:  LATTICE
    Target Device:  LCMXO2-1200ZECSBGA132
    Target Performance:   3
    Mapper:  xo2c00,  version:  Diamond Version 2.0.0.154
    Mapped on:  07/24/12  16:13:51

    Design Summary
       Number of registers:    634
          PFU registers:    628
          PIO registers:    6
       Number of SLICEs:           640 out of   640 (100%)
          SLICEs(logic/ROM):       160 out of   160 (100%)
          SLICEs(logic/ROM/RAM):   480 out of   480 (100%)
              As RAM:           48 out of   480 (10%)
              As Logic/ROM:    432 out of   480 (90%)
       Number of logic LUT4s:     784
       Number of distributed RAM:  48 (96 LUT4s)
       Number of ripple logic:    186 (372 LUT4s)
       Number of shift registers:   0
       Total number of LUT4s:     1252
       Number of PIO sites used: 36 out of 105 (34%)
          Number of PIO sites used for single ended IOs: 32
          Number of PIO sites used for differential IOs: 4 (represented by 2 PIO
         comps in NCD)
       Number of block RAMs:  6 out of 7 (86%)
       Number of GSRs:  1 out of 1 (100%)
       EFB used :       Yes
       JTAG used :      No
       Readback used :  No
       Oscillator used :  Yes
       Startup used :   No
       POR :            On
       Bandgap :        On
       Number of Power Controller:  1 out of 1 (100%)
       Number of Dynamic Bank Controller (BCINRD):  1 out of 4 (25%)
       Number of Dynamic Bank Controller (BCLVDSO):  0 out of 1 (0%)
       Number of DCCA:  0 out of 8 (0%)
       Number of DCMA:  0 out of 2 (0%)
       Number of PLLs:  0 out of 1 (0%)
       Number of DQSDLLs:  0 out of 2 (0%)
       Number of CLKDIVC:  0 out of 4 (0%)
       Number of ECLKSYNCA:  0 out of 4 (0%)
       Number of ECLKBRIDGECS:  0 out of 2 (0%)
       Notes:-
          1. Total number of LUT4s = (Number of logic LUT4s) + 2*(Number of
         distributed RAMs) + 2*(Number of ripple logic)
          2. Number of logic LUT4s does not include count of distributed RAM and
         ripple logic.

       Number of clocks:  15
         Net GND: 1 loads, 1 rising, 0 falling (Driver: GND )
         Net clk: 288 loads, 288 rising, 0 falling (Driver:
         clkselect_wb_inst/clk_switch_inst1/out_clk )
         Net DebounceRingOSCb_c[0]: 16 loads, 16 rising, 0 falling (Driver:
         DebounceRingOSCb_RNO[0] )
         Net lcdstate_225: 4 loads, 4 rising, 0 falling (Driver: lcdstate_s0_0_a2 )
         Net ButtonPushed: 2 loads, 0 rising, 2 falling (Driver:
         PushButton_Debouncer_inst/Pushed )
         Net EFB_Inst/i2c1_scli: 1 loads, 1 rising, 0 falling (Driver: PIO scl )
         Net EFB_Inst/spi_clk_i: 1 loads, 1 rising, 0 falling (Driver: PIO spi_sclk
         )
         Net clk_USB_c: 70 loads, 70 rising, 0 falling (Driver: PIO clk_USB )
         Net clkselect_wb_inst/RingOSCclk: 2 loads, 2 rising, 0 falling (Driver:
         clkselect_wb_inst/oscclkclean_inst/RingOSCclk )
         Net clkselect_wb_inst/oscclk: 6 loads, 6 rising, 0 falling (Driver:
         clkselect_wb_inst/OSCH_inst )
         Net clkselect_wb_inst/RingOSCraw_c: 20 loads, 20 rising, 0 falling (Driver:
         clkselect_wb_inst/RingOSC_inst/RingOSCb_RNO[0] )
         Net ToggleUSERSTDBY_i: 1 loads, 1 rising, 0 falling (Driver: USERSTDBY_RNO
         )
         Net lcdstate[3]: 4 loads, 4 rising, 0 falling (Driver:
         lcdstate_derived_clock_RNO[3] )
         Net lcdstate[2]: 4 loads, 4 rising, 0 falling (Driver: lcdstate_s2_0_a2 )
         Net lcdstate_226: 4 loads, 4 rising, 0 falling (Driver: lcdstate_s1_0_a2 )
       Number of Clock Enables:  61
         Net un1_state_0_sqmuxa_0: 1 loads, 1 LSLICEs
         Net PushButton_Debouncer_inst/un1_Pushed8: 1 loads, 1 LSLICEs
         Net lcdcounter_RNIA65L[0]: 12 loads, 12 LSLICEs
         Net lcdcounter_2_cry_11_0_RNI9V2D: 12 loads, 12 LSLICEs
         Net capsense_inst/SampleCounterCO: 2 loads, 2 LSLICEs
         Net capsense_inst/FastCounter4Sample_0_sqmuxa: 4 loads, 4 LSLICEs
         Net capsense_inst/N_424_i: 4 loads, 4 LSLICEs
         Net capsense_inst/N_867_i: 4 loads, 4 LSLICEs
         Net capsense_inst/N_425_i: 4 loads, 4 LSLICEs
         Net capsense_inst/FastCounter2e: 4 loads, 4 LSLICEs
         Net capsense_inst/N_866_i: 4 loads, 4 LSLICEs
         Net capsense_inst/FastCounter1e: 4 loads, 4 LSLICEs
         Net capsense_inst/FastCounter1Sample_0_sqmuxa: 4 loads, 4 LSLICEs
         Net STRING_TABLE_INST/EXT_ROM_INST_RNO: 2 loads, 0 LSLICEs
         Net adc_wb_inst/adc_inst/SSD_ADC/rollover: 4 loads, 4 LSLICEs
         Net adc_wb_inst/adc_inst/SSD_ADC/box_ave/latch_result: 4 loads, 4 LSLICEs
         Net adc_wb_inst/adc_inst/SSD_ADC/box_ave/accumulate: 6 loads, 6 LSLICEs
         Net adc_wb_inst/adc_inst/SSD_ADC/sigmae: 6 loads, 6 LSLICEs
         Net adc_wb_inst/PowerRail5: 1 loads, 1 LSLICEs
         Net UART_INST/u_txmitt/tx_state[0]: 10 loads, 10 LSLICEs
         Net UART_INST/u_txmitt/tx_state_5_0_a2: 5 loads, 5 LSLICEs
         Net UART_INST/u_txmitt/un1_thr_wr_1: 1 loads, 1 LSLICEs
         Net UART_INST/u_txmitt/un1_tsr_empty5: 1 loads, 1 LSLICEs
         Net UART_INST/u_rxcver/un1_cs_state_2_i: 1 loads, 1 LSLICEs
         Net UART_INST/u_rxcver/un1_databit_recved_num_1_sqmuxa_0: 1 loads, 1
         LSLICEs
         Net UART_INST/u_rxcver/databit_recved_nume: 6 loads, 6 LSLICEs
         Net UART_INST/u_rxcver/N_618_i: 4 loads, 4 LSLICEs
         Net UART_INST/u_rxcver/un1_hunt_1_0: 1 loads, 1 LSLICEs
         Net UART_INST/u_rxcver/un1_cs_state_0_sqmuxa_2_i_s: 1 loads, 1 LSLICEs

         Net UART_INST/u_rxcver/un1_lsr_rd: 4 loads, 4 LSLICEs
         Net UART_INST/u_rxcver/N_616_i: 1 loads, 1 LSLICEs
         Net UART_INST/data_8bit17: 8 loads, 8 LSLICEs
         Net UART_INST/u_intface/thr_nonfifo_0_sqmuxa: 4 loads, 4 LSLICEs
         Net UART_INST/u_intface/lcr_1_sqmuxa: 4 loads, 4 LSLICEs
         Net UART_INST/u_intface/ier_1_sqmuxa: 2 loads, 2 LSLICEs
         Net UART_INST/u_intface/div_wr_strobe: 4 loads, 4 LSLICEs
         Net lm8_inst/u1_isp8/addr_cyc: 7 loads, 7 LSLICEs
         Net lm8_inst/u1_isp8/data_cyc: 6 loads, 6 LSLICEs
         Net lm8_inst/u1_isp8/u1_isp8_flow_cntl/zero_flag13: 1 loads, 1 LSLICEs
         Net lm8_inst/u1_isp8/u1_isp8_flow_cntl/carry_flag_int12: 1 loads, 1 LSLICEs
         Net lm8_inst/u1_isp8/N_982_i: 9 loads, 1 LSLICEs
         Net lm8_inst/u1_isp8/page_ptr25: 2 loads, 2 LSLICEs
         Net lm8_inst/u1_isp8/page_ptr16: 1 loads, 1 LSLICEs
         Net clkselect_wb_inst/CalbrateRingOSC: 12 loads, 12 LSLICEs
         Net clkselect_wb_inst/oscclkclean_inst/CalbrateRingOSC_0_sqmuxa: 5 loads, 5
         LSLICEs
         Net clkselect_wb_inst/SelectClockwb5: 1 loads, 1 LSLICEs
         Net clkselect_wb_inst/N_36: 1 loads, 1 LSLICEs
         Net clkselect_wb_inst/RingOSCEnbDelaye: 3 loads, 3 LSLICEs
         Net clkselect_wb_inst/OSCEnbDelaye: 3 loads, 3 LSLICEs
         Net clkselect_wb_inst/OSCEnb1_1_sqmuxa_i: 1 loads, 1 LSLICEs
         Net lcd_sw_inst/LCD1_0_sqmuxa: 4 loads, 4 LSLICEs
         Net lcd_sw_inst/LCDDP1_1_sqmuxa: 1 loads, 1 LSLICEs
         Net lcd_sw_inst/LCD2_1_sqmuxa: 4 loads, 4 LSLICEs
         Net lcd_sw_inst/LCDEnWB_1_sqmuxa: 1 loads, 1 LSLICEs
         Net lcd_sw_inst/LCDDP3_1_sqmuxa: 1 loads, 1 LSLICEs
         Net lcd_sw_inst/LCDDP2_1_sqmuxa: 1 loads, 1 LSLICEs
         Net lcd_sw_inst/LCDCol_1_sqmuxa: 1 loads, 1 LSLICEs
         Net lcd_sw_inst/LCD4_1_sqmuxa: 4 loads, 4 LSLICEs
         Net lcd_sw_inst/LCD3_1_sqmuxa: 4 loads, 4 LSLICEs
         Net reset_gen_inst/reset_counter11: 2 loads, 2 LSLICEs
         Net lcdstate_118_0_a2: 1 loads, 1 LSLICEs
       Number of local set/reset loads for net wb_rst merged into GSR:  181
       Number of LSRs:  11
         Net PushBn_c: 2 loads, 2 LSLICEs
         Net clk: 1 loads, 1 LSLICEs
         Net USERSTDBY: 16 loads, 16 LSLICEs
         Net rst_c: 105 loads, 103 LSLICEs
         Net STDBY: 6 loads, 2 LSLICEs
         Net capsense_inst/Recalibrate: 39 loads, 39 LSLICEs
         Net wb_rst: 7 loads, 5 LSLICEs
         Net lm8_inst/u1_isp8/rst_n_reg: 43 loads, 43 LSLICEs
         Net lm8_rst: 1 loads, 1 LSLICEs
         Net clkselect_wb_inst/clk_switch_inst1/capture2: 1 loads, 1 LSLICEs
         Net clkselect_wb_inst/clk_switch_inst1/capture1: 1 loads, 1 LSLICEs
       Number of nets driven by tri-state buffers:  0
       Top 10 highest fanout non-clock nets:
         Net rst_c: 108 loads
         Net addr[1]: 49 loads
         Net lm8_inst/u1_isp8/rst_n_reg: 44 loads
         Net addr[0]: 42 loads
         Net addr[2]: 42 loads
         Net capsense_inst/Recalibrate: 39 loads
         Net UART_INST/u_rxcver/cs_state[0]: 33 loads
         Net capsense_inst/FastCounter4: 32 loads

         Net lm8_inst/u1_isp8/u1_isp8_prom/raddr10_ff: 30 loads
         Net state[1]: 30 loads

       Number of warnings:  30
       Number of errors:    0

    Design Errors/Warnings

    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (43): Error in LOCATE
         COMP "FastCounterOut" SITE "N6" ;
    : COMP "FastCounterOut" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (44): Error in LOCATE
         COMP "SampleCounterOut" SITE "A13" ;
    : COMP "SampleCounterOut" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (45): Error in LOCATE
         COMP "SampleTime1out" SITE "P6" ;
    : COMP "SampleTime1out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (46): Error in LOCATE
         COMP "FastCounter1out" SITE "N6" ;
    : COMP "FastCounter1out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (47): Error in LOCATE
         COMP "SampleTime2out" SITE "A13" ;
    : COMP "SampleTime2out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (48): Error in LOCATE
         COMP "FastCounter2out" SITE "B13" ;
    : COMP "FastCounter2out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (49): Error in LOCATE
         COMP "SampleTime3out" SITE "C10" ;
    : COMP "SampleTime3out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (50): Error in LOCATE
         COMP "FastCounter3out" SITE "B9" ;
    : COMP "FastCounter3out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (51): Error in LOCATE
         COMP "SampleTime4out" SITE "H12" ;
    : COMP "SampleTime4out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (52): Error in LOCATE
         COMP "FastCounter4out" SITE "G13" ;
    : COMP "FastCounter4out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (53): Error in LOCATE
         COMP "SampleCounterOut" SITE "D1" ;
    : COMP "SampleCounterOut" not found in design. Disabled this preference.

    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (55): Error in LOCATE
         COMP "USBorBattout" SITE "D1" ;
    : COMP "USBorBattout" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (56): Error in LOCATE
         COMP "touched1out" SITE "C2" ;
    : COMP "touched1out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (57): Error in LOCATE
         COMP "touched2out" SITE "C3" ;
    : COMP "touched2out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (58): Error in LOCATE
         COMP "touched3out" SITE "C1" ;
    : COMP "touched3out" not found in design. Disabled this preference.
    WARNING: C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_En
         vironment_Scanning/project/Environment_Scanning.lpf (59): Error in LOCATE
         COMP "touched4out" SITE "B2" ;
    : COMP "touched4out" not found in design. Disabled this preference.
    WARNING: Preference parsing results:  16 semantic errors detected
    WARNING: There are errors in the preference file, "C:/asdf/MachXO2 Pico Demo
         from Website/doc41117x92/Demo_MachXO2_Pico_Environment_Scanning/project/Env
         ironment_Scanning.lpf".
    WARNING: EFB_Inst/EFBInst_0: SLAVE_SPI_PORT was set to ENABLE by ngdbuild
         generated property. Setting in preference file was ignored.
    WARNING: EFB_Inst/EFBInst_0: I2C_PORT was set to ENABLE by ngdbuild generated
         property. Setting in preference file was ignored.
    WARNING: Using local reset signal 'wb_rst' to infer global GSR net.
    WARNING: BANDGAP turned off dynamically by Power controller
         'PowerCntr_inst/PCNTR_Inst0'. When the BANDGAP circuitry is turned off, POR
         circuitry, analog circuits PLL, oscillator, Inputs (SSTLXX, HSTL18,
         LVCMOSXXD, SSTLXXD,HSTL18D, LVTTL33D, LVCMOSXXRXX, LVDS25, RSDS25, BLVDS25,
         MLVDS25 and LVPECL33), Outputs (LVDS25 true only), Bidir (SSTLXX, HSTL18 ,
         LVCMOSXXD, SSTLXXD, HSTL18D, LVTTL33D, BLVDS25E and MLVDS25E) are turned
         off.
    WARNING: POR turned off dynamically by Power controller
         'PowerCntr_inst/PCNTR_Inst0'. POR is only released when SFLAG is cleared.
    WARNING: Power controller 'PowerCntr_inst/PCNTR_Inst0' USERSTDBY wake signal
         'USERSTDBY' is controlled via logic driven by oscillator component
         'clkselect_wb_inst/OSCH_inst' which will be disabled when BANDGAP is turned
         off.
    WARNING: Power controller 'PowerCntr_inst/PCNTR_Inst0' dynamic BANDGAP option is
         enabled. The design contains input and/or bidirectional buffer(s) with
         following IO_TYPES that will be disabled when BANDGAP is turned off:
         LVDS25.
    WARNING: Power controller 'PowerCntr_inst/PCNTR_Inst0' dynamic BANDGAP option is
         enabled. The design contains oscillator component which will be disabled
         when BANDGAP is turned off.
    WARNING: The reset of EBR
         'lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_1_1_0' cannot
         be controlled. The local reset is not connected to any control signal and
         set to GND. The global reset is disabled via GSR property. To control the
         EBR reset, either connect the local reset to a control signal or force the
         GSR property to be enabled.
    WARNING: The reset of EBR

         'lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_0_0_3' cannot
         be controlled. The local reset is not connected to any control signal and
         set to GND. The global reset is disabled via GSR property. To control the
         EBR reset, either connect the local reset to a control signal or force the
         GSR property to be enabled.
    WARNING: The reset of EBR
         'lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_0_1_2' cannot
         be controlled. The local reset is not connected to any control signal and
         set to GND. The global reset is disabled via GSR property. To control the
         EBR reset, either connect the local reset to a control signal or force the
         GSR property to be enabled.
    WARNING: The reset of EBR
         'lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_1_0_1' cannot
         be controlled. The local reset is not connected to any control signal and
         set to GND. The global reset is disabled via GSR property. To control the
         EBR reset, either connect the local reset to a control signal or force the
         GSR property to be enabled.

    IO (PIO) Attributes

    +---------------------+-----------+-----------+------------+
    | IO Name             | Direction | Levelmode | IO         |
    |                     |           |  IO_TYPE  | Register   |
    +---------------------+-----------+-----------+------------+
    | cap_btn1            | BIDIR     | LVCMOS25  | TRI        |
    +---------------------+-----------+-----------+------------+
    | LCD_COM0            | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | spi_csn             | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | PushBn              | INPUT     | LVCMOS25  | IN         |
    +---------------------+-----------+-----------+------------+
    | Icco_analog_cmp_p   | INPUT     | LVDS25    |            |
    +---------------------+-----------+-----------+------------+
    | spi_mosi            | BIDIR     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | spi_miso            | BIDIR     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | spi_sclk            | BIDIR     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | sda                 | BIDIR     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | scl                 | BIDIR     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | clk_USB             | INPUT     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | Icco_analog_out     | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | Icc_analog_out      | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | EnTempSPI           | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | EnAMP               | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | I2CAlert            | OUTPUT    | LVCMOS25  |            |

    +---------------------+-----------+-----------+------------+
    | uart_tx             | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | uart_rx             | INPUT     | LVCMOS25  | IN         |
    +---------------------+-----------+-----------+------------+
    | LCD_12              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_11              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_10              | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_9               | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_8               | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_7               | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_6               | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_5               | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_COM3            | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_COM2            | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | LCD_COM1            | OUTPUT    | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | cap_btn4            | BIDIR     | LVCMOS25  | TRI        |
    +---------------------+-----------+-----------+------------+
    | cap_btn3            | BIDIR     | LVCMOS25  | TRI        |
    +---------------------+-----------+-----------+------------+
    | cap_btn2            | BIDIR     | LVCMOS25  | TRI        |
    +---------------------+-----------+-----------+------------+
    | rst                 | INPUT     | LVCMOS25  |            |
    +---------------------+-----------+-----------+------------+
    | Icc_analog_cmp_p    | INPUT     | LVDS25    |            |
    +---------------------+-----------+-----------+------------+

    Removed logic

    Block lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/scuba_vlo_inst undriven
         or does not drive anything - clipped.
    Block lm8_inst/U2_scratchpad/scuba_vlo_inst undriven or does not drive anything
         - clipped.
    Block lm8_inst/u1_isp8/genblk8.u2_isp8_rfmem/scuba_vlo_inst undriven or does not
         drive anything - clipped.
    Block lm8_inst/u1_isp8/genblk7.u1_isp8_rfmem/scuba_vlo_inst undriven or does not
         drive anything - clipped.
    Block lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/scuba_vhi_inst undriven or does
         not drive anything - clipped.
    Block lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/addsubd undriven or does not drive
         anything - clipped.
    Block lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/mem_0_0/RAM1 undriven or
         does not drive anything - clipped.
    Signal PushBn_c_i was merged into signal PushBn_c

    Signal clkselect_wb_inst/oscclkclean_inst/CalbrateRingOSC_i was merged into
         signal clkselect_wb_inst/CalbrateRingOSC
    Signal clkselect_wb_inst/clk_switch_inst1/capture2_i was merged into signal
         clkselect_wb_inst/clk_switch_inst1/capture2
    Signal clkselect_wb_inst/clk_switch_inst1/capture1_i was merged into signal
         clkselect_wb_inst/clk_switch_inst1/capture1
    Signal lm8_inst/u1_isp8/rst_n_reg_i was merged into signal
         lm8_inst/u1_isp8/rst_n_reg
    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/add_sub_inv was merged into
         signal lm8_inst/u1_isp8/u1_isp8_alu/N_767_i
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/dec0_wre3 was merged
         into signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/N_876_i
    Signal UART_INST/u_txmitt/tx_state_i[0] was merged into signal
         UART_INST/u_txmitt/tx_state[0]
    Signal capsense_inst/Recalibrate_i was merged into signal
         capsense_inst/Recalibrate
    Signal ButtonPushed_i was merged into signal ButtonPushed
    Signal lm8_inst/U2_scratchpad/scuba_vhi undriven or does not drive anything -
         clipped.
    Signal lm8_inst/u1_isp8/genblk8.u2_isp8_rfmem/scuba_vhi undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/genblk7.u1_isp8_rfmem/scuba_vhi undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_prom/scuba_vlo undriven or does not drive
         anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_prom/scuba_vhi undriven or does not drive
         anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/scuba_vlo undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/scuba_vhi undriven or
         does not drive anything - clipped.
    Signal STRING_TABLE_INST/EXT_ROM_INST/scuba_vlo undriven or does not drive
         anything - clipped.
    Signal STRING_TABLE_INST/EXT_ROM_INST/scuba_vhi undriven or does not drive
         anything - clipped.
    Signal un7_NextStateDelay_1_cry_23_0_COUT undriven or does not drive anything -
         clipped.
    Signal lcdcounter_3_cry_0_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_3_cry_1_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_3_s_11_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_3_s_11_0_COUT undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_0_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_0_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_1_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_1_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_3_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_3_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_5_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_5_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_7_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_7_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_9_0_S1 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_9_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_11_0_S0 undriven or does not drive anything - clipped.
    Signal lcdcounter_2_cry_11_0_COUT undriven or does not drive anything - clipped.
    Signal clkselect_wb_inst/OSCEnbDelay_cry_0_S0[0] undriven or does not drive

         anything - clipped.
    Signal clkselect_wb_inst/OSCEnbDelay_cry_0_COUT[3] undriven or does not drive
         anything - clipped.
    Signal clkselect_wb_inst/RingOSCEnbDelay_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal clkselect_wb_inst/RingOSCEnbDelay_cry_0_COUT[3] undriven or does not
         drive anything - clipped.
    Signal clkselect_wb_inst/SEDSTDBY undriven or does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/CalRingOSCcnt_cry_0_S0[0] undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/CalRingOSCcnt_s_0_S1[9] undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/CalRingOSCcnt_s_0_COUT[9] undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_0_0_S1 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_0_0_S0 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_1_0_S1 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_1_0_S0 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_3_0_S1 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_3_0_S0 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_5_0_S1 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_5_0_S0 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_7_0_S1 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_7_0_S0 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_8_0_S1 undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/un1_RingOSCcnt_cry_8_0_COUT undriven
         or does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/RingOSCcnt_cry_0_S0[0] undriven or
         does not drive anything - clipped.
    Signal clkselect_wb_inst/oscclkclean_inst/RingOSCcnt_cry_0_COUT[7] undriven or
         does not drive anything - clipped.
    Signal lm8_inst/U2_scratchpad/scuba_vlo undriven or does not drive anything -
         clipped.
    Signal lm8_inst/u1_isp8/genblk8.u2_isp8_rfmem/scuba_vlo undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/genblk7.u1_isp8_rfmem/scuba_vlo undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/scuba_vhi undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/addsub_0/S0 undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/addsubd/S1 undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/co4d undriven or does not drive
         anything - clipped.

    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/addsubd/COUT undriven or does not
         drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/co4 undriven or does not drive
         anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/un1_stack_ptr_cry_0_0_S1 undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/un1_stack_ptr_cry_0_0_S0 undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/un1_stack_ptr_s_3_0_S1 undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/un1_stack_ptr_s_3_0_COUT undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/un11_pc_int_cry_0_0_S1 undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/un11_pc_int_cry_0_0_S0 undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/un11_pc_int_cry_9_0_COUT undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/mem_0_0/DO2 undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/mem_0_0/DO3 undriven or
         does not drive anything - clipped.
    Signal lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/mem_0_0/DO1 undriven or
         does not drive anything - clipped.
    Signal UART_INST/u_rxcver/un1_counter_1_i[0] undriven or does not drive anything
         - clipped.
    Signal UART_INST/u_rxcver/un1_counter_2_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/un1_counter_2_s_15_0_S1 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/un1_counter_2_s_15_0_COUT undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_N_37 undriven or does not drive anything
         - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_1_0_S0 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_9_0_S1 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_9_0_S0 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_27_0_S1 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_27_0_S0 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_33_0_S1 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_33_0_S0 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_21_0_S0 undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_rxcver/cs_state12_0_I_21_0_COUT undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_txmitt/counter_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal UART_INST/u_txmitt/counter_s_0_S1[15] undriven or does not drive anything
         - clipped.

    Signal UART_INST/u_txmitt/counter_s_0_COUT[15] undriven or does not drive
         anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/counter_cry_0_S0[0] undriven or does not
         drive anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/counter_s_0_S1[9] undriven or does not drive
         anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/counter_s_0_COUT[9] undriven or does not
         drive anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/sigma_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/sigma_s_0_S1[9] undriven or does not drive
         anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/sigma_s_0_COUT[9] undriven or does not drive
         anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/box_ave/un6_accum_cry_0_0_S1 undriven or
         does not drive anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/box_ave/un6_accum_cry_0_0_S0 undriven or
         does not drive anything - clipped.
    Signal adc_wb_inst/adc_inst/SSD_ADC/box_ave/un6_accum_cry_9_0_COUT undriven or
         does not drive anything - clipped.
    Signal EFB_Inst/CFGSTDBY undriven or does not drive anything - clipped.
    Signal EFB_Inst/CFGWAKE undriven or does not drive anything - clipped.
    Signal EFB_Inst/WBCUFMIRQ undriven or does not drive anything - clipped.
    Signal EFB_Inst/TCOC undriven or does not drive anything - clipped.
    Signal EFB_Inst/TCINT undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIIRQO undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPICSNEN undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIMCSN7 undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIMCSN6 undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIMCSN5 undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIMCSN4 undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIMCSN3 undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIMCSN2 undriven or does not drive anything - clipped.
    Signal EFB_Inst/SPIMCSN1 undriven or does not drive anything - clipped.
    Signal EFB_Inst/I2C2IRQO undriven or does not drive anything - clipped.
    Signal EFB_Inst/I2C1IRQO undriven or does not drive anything - clipped.
    Signal EFB_Inst/I2C2SDAOEN undriven or does not drive anything - clipped.
    Signal EFB_Inst/I2C2SDAO undriven or does not drive anything - clipped.
    Signal EFB_Inst/I2C2SCLOEN undriven or does not drive anything - clipped.
    Signal EFB_Inst/I2C2SCLO undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO0 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO1 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO2 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO3 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO4 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO5 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO6 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLDATO7 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLADRO0 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLADRO1 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLADRO2 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLADRO3 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLADRO4 undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLWEO undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLL1STBO undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLL0STBO undriven or does not drive anything - clipped.

    Signal EFB_Inst/PLLRSTO undriven or does not drive anything - clipped.
    Signal EFB_Inst/PLLCLKO undriven or does not drive anything - clipped.
    Signal capsense_inst/FastCounter1_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/FastCounter1_cry_0_COUT[5] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/FastCounter2_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/FastCounter2_cry_0_COUT[5] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/FastCounter3_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/FastCounter3_cry_0_COUT[5] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/FastCounter4_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/FastCounter4_cry_0_COUT[5] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/SampleCounter_cry_0_S0[0] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/SampleCounter_s_0_S1[7] undriven or does not drive anything
         - clipped.
    Signal capsense_inst/SampleCounter_s_0_COUT[7] undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_2_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_2_s_7_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_2_s_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_2_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_2_s_7_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_2_s_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_2_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_2_s_7_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_2_s_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_2_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_2_s_7_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_2_s_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_0_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_1_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_1_0_S0 undriven or does not drive
         anything - clipped.

    Signal capsense_inst/un1_FastCounter3_4_cry_3_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_3_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_5_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_5_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_7_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter3_4_cry_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_0_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_1_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_1_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_3_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_3_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_5_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_5_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_7_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter2_4_cry_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_0_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_0_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_1_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_1_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_3_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_3_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_5_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_5_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_7_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter1_4_cry_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_0_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_0_0_S0 undriven or does not drive
         anything - clipped.

    Signal capsense_inst/un1_FastCounter4_4_cry_1_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_1_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_3_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_3_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_5_0_S1 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_5_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_7_0_S0 undriven or does not drive
         anything - clipped.
    Signal capsense_inst/un1_FastCounter4_4_cry_7_0_COUT undriven or does not drive
         anything - clipped.
    Signal capsense_inst/touched48_cry_0_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_0_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_1_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_1_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_3_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_3_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_5_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_5_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_7_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched48_cry_7_0_COUT undriven or does not drive anything
         - clipped.
    Signal capsense_inst/touched38_cry_0_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_0_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_1_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_1_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_3_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_3_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_5_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_5_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_7_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched38_cry_7_0_COUT undriven or does not drive anything
         - clipped.

    Signal capsense_inst/touched28_cry_0_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_0_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_1_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_1_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_3_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_3_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_5_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_5_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_7_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched28_cry_7_0_COUT undriven or does not drive anything
         - clipped.
    Signal capsense_inst/touched18_cry_0_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_0_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_1_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_1_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_3_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_3_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_5_0_S1 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_5_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_7_0_S0 undriven or does not drive anything -
         clipped.
    Signal capsense_inst/touched18_cry_7_0_COUT undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB8 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB7 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB6 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB5 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB4 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB3 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB2 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB1 undriven or does not drive anything
         - clipped.

    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOB0 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOA8 undriven or does not drive anything
         - clipped.
    Signal LCDCharMap_inst/LCDCharMap_0_0_0_DOA7 undriven or does not drive anything
         - clipped.
    Signal PowerCntr_inst/SFLAG undriven or does not drive anything - clipped.
    Signal PowerCntr_inst/STOP undriven or does not drive anything - clipped.
    Signal un7_NextStateDelay_1_cry_0_0_S1 undriven or does not drive anything -
         clipped.
    Signal un7_NextStateDelay_1_cry_0_0_S0 undriven or does not drive anything -
         clipped.
    Block PushBn_pad_RNI0NAD was optimized away.
    Block clkselect_wb_inst/oscclkclean_inst/CalbrateRingOSC_RNI1DV5 was optimized
         away.
    Block clkselect_wb_inst/clk_switch_inst1/transfer2_RNO was optimized away.
    Block clkselect_wb_inst/clk_switch_inst1/transfer1_RNO was optimized away.
    Block lm8_inst/u1_isp8/rst_n_reg_RNIQKL6 was optimized away.
    Block lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/INV_0 was optimized away.
    Block lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/LUT4_0 was optimized
         away.
    Block UART_INST/u_txmitt/genblk2.genblk1.tx_state_RNISRIB[0] was optimized away.
    Block capsense_inst/Recalibrate_RNI3U was optimized away.
    Block PushButton_Debouncer_inst/Pushed_RNIQABE was optimized away.
    Block lm8_inst/U2_scratchpad/scuba_vhi_inst was optimized away.
    Block lm8_inst/u1_isp8/genblk8.u2_isp8_rfmem/scuba_vhi_inst was optimized away.
    Block lm8_inst/u1_isp8/genblk7.u1_isp8_rfmem/scuba_vhi_inst was optimized away.
    Block lm8_inst/u1_isp8/u1_isp8_prom/scuba_vlo_inst was optimized away.
    Block lm8_inst/u1_isp8/u1_isp8_prom/scuba_vhi_inst was optimized away.
    Block lm8_inst/u1_isp8/u1_isp8_alu/u1_addsub8/scuba_vlo_inst was optimized away.
    Block lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/scuba_vhi_inst was
         optimized away.
    Block STRING_TABLE_INST/EXT_ROM_INST/scuba_vlo_inst was optimized away.
    Block STRING_TABLE_INST/EXT_ROM_INST/scuba_vhi_inst was optimized away.

    Memory Usage

    /LCDCharMap_inst:
        EBRs: 1
        RAM SLICEs: 0
        Logic SLICEs: 0
        PFU Registers: 0
        -Contains EBR LCDCharMap_0_0_0:  TYPE= DP8KC,  Width_A= 7,  Depth_A= 256,
             REGMODE_A= OUTREG,  REGMODE_B= NOREG,  RESETMODE= SYNC,
             ASYNC_RESET_RELEASE= SYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B= NORMAL,
             GSR= DISABLED,  MEM_INIT_FILE= lcdcharmap.mem,  MEM_LPC_FILE=
             LCDCharMap.lpc
    /STRING_TABLE_INST/EXT_ROM_INST:
        EBRs: 1
        RAM SLICEs: 0
        Logic SLICEs: 0
        PFU Registers: 0
        -Contains EBR pmi_romXhmenusdn8101024_0_0_0:  TYPE= DP8KC,  Width_A= 8,
             Depth_A= 1024,  REGMODE_A= NOREG,  REGMODE_B= NOREG,  RESETMODE= SYNC,
             ASYNC_RESET_RELEASE= SYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B= NORMAL,

             GSR= DISABLED,  MEM_INIT_FILE= menu.hex,  MEM_LPC_FILE=
             pmi_romXhmenusdn8101024__PMIR__1024__8__8H
    /lm8_inst/U2_scratchpad:
        EBRs: 0
        RAM SLICEs: 12
        Logic SLICEs: 0
        PFU Registers: 11
    /lm8_inst/u1_isp8/genblk7.u1_isp8_rfmem:
        EBRs: 0
        RAM SLICEs: 12
        Logic SLICEs: 1
        PFU Registers: 0
    /lm8_inst/u1_isp8/genblk8.u2_isp8_rfmem:
        EBRs: 0
        RAM SLICEs: 12
        Logic SLICEs: 1
        PFU Registers: 0
    /lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem:
        EBRs: 0
        RAM SLICEs: 11
        Logic SLICEs: 0
        PFU Registers: 0
    /lm8_inst/u1_isp8/u1_isp8_flow_cntl/u1_isp8_stkmem/mem_0_0/RAMW:
        EBRs: 0
        RAM SLICEs: 1
        Logic SLICEs: 0
        PFU Registers: 0
    /lm8_inst/u1_isp8/u1_isp8_prom:
        EBRs: 4
        RAM SLICEs: 0
        Logic SLICEs: 0
        PFU Registers: 0
        -Contains EBR pmi_romXhprom_initadn18112048_1_1_0:  TYPE= DP8KC,  Width_A=
             9,  Depth_A= 1024,  REGMODE_A= NOREG,  REGMODE_B= NOREG,  RESETMODE=
             ASYNC,  ASYNC_RESET_RELEASE= ASYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B=
             NORMAL,  GSR= DISABLED,  MEM_INIT_FILE= prom_init.hex,  MEM_LPC_FILE=
             pmi_romXhprom_initadn18112048__PMIR__2048__18__18H
        -Contains EBR pmi_romXhprom_initadn18112048_0_0_3:  TYPE= DP8KC,  Width_A=
             9,  Depth_A= 1024,  REGMODE_A= NOREG,  REGMODE_B= NOREG,  RESETMODE=
             ASYNC,  ASYNC_RESET_RELEASE= ASYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B=
             NORMAL,  GSR= DISABLED,  MEM_INIT_FILE= prom_init.hex,  MEM_LPC_FILE=
             pmi_romXhprom_initadn18112048__PMIR__2048__18__18H
        -Contains EBR pmi_romXhprom_initadn18112048_0_1_2:  TYPE= DP8KC,  Width_A=
             9,  Depth_A= 1024,  REGMODE_A= NOREG,  REGMODE_B= NOREG,  RESETMODE=
             ASYNC,  ASYNC_RESET_RELEASE= ASYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B=
             NORMAL,  GSR= DISABLED,  MEM_INIT_FILE= prom_init.hex,  MEM_LPC_FILE=
             pmi_romXhprom_initadn18112048__PMIR__2048__18__18H
        -Contains EBR pmi_romXhprom_initadn18112048_1_0_1:  TYPE= DP8KC,  Width_A=
             9,  Depth_A= 1024,  REGMODE_A= NOREG,  REGMODE_B= NOREG,  RESETMODE=
             ASYNC,  ASYNC_RESET_RELEASE= ASYNC,  WRITEMODE_A= NORMAL,  WRITEMODE_B=
             NORMAL,  GSR= DISABLED,  MEM_INIT_FILE= prom_init.hex,  MEM_LPC_FILE=
             pmi_romXhprom_initadn18112048__PMIR__2048__18__18H

    Power Controller Summary
    ------------------------

      PCNTR Instance Name:                              PowerCntr_inst/PCNTR_Inst0
      Entry Options:
            Configuration:                              DISABLED
            User:                                       ENABLED/USERSTDBY
             Stop to Standby Delay:                     Bypass
      Wake Options:
            Configuration:                              DISABLED
            User:                                       ENABLED/USERSTDBY_i
            Timeout Counter:                            DISABLED
                  Bypass:                               ENABLED
      Standby Options:
            Turn Off POR:                               ENABLED
            Turn Off Bandgap:                           ENABLED

    Dynamic Bank Controller Summary
    -------------------------------

      BCINRD Instance Name:                             BankController_inst/InRD_2
      BANK:                                             2
      Control Signal:                                   STDBY

    OSC Summary
    -----------

    OSC 1:                                     Pin/Node Value
      OSC Instance Name:                                clkselect_wb_inst/OSCH_inst
      OSC Type:                                         OSCH
      STDBY Input:                             NODE     clkselect_wb_inst/OSCEnb
      OSC Output:                              NODE     clkselect_wb_inst/oscclk
      OSC Nominal Frequency (MHz):                      2.08

    Embedded Functional Block Connection Summary:
    ---------------------------------------------

       Desired WISHBONE clock frequency: 2.0 MHz
       Clock source:                     clk
       Reset source:                     wb_rst
       Functions mode:
          I2C #1 (Primary) Function:     ENABLED
          I2C #2 (Secondary) Function:   DISABLED
          SPI Function:                  ENABLED
          Timer/Counter Function:        DISABLED
          Timer/Counter Mode:            WB
          UFM Connection:                DISABLED
          PLL0 Connection:               DISABLED
          PLL1 Connection:               DISABLED
       I2C Function Summary:
       --------------------
          I2C Component:          PRIMARY
          I2C Addressing:         7BIT
          I2C Performance:        100kHz
          Slave Address:          0b0001001
          General Call:           ENABLED

          I2C Wake Up:            DISABLED
          I2C Component:          UFM/Configuration
          I2C Addressing:         7BIT
          I2C Performance:        100kHz
          Slave Address:          0b0001000
       SPI Function Summary:
       --------------------
          SPI Mode:               BOTH
          SPI Data Order:         LSB to MSB
          SPI Clock Inversion:    DISABLED
          SPI Phase Adjust:       DISABLED
          SPI Wakeup:             DISABLED
       Timer/Counter Function Summary:
       ------------------------------
          None
       UFM Function Summary:
       --------------------
          UFM Utilization:        General Purpose Flash Memory
          Available General
          Purpose Flash Memory:   511 Pages (511*128 Bits)

          EBR Blocks with Unique
          Initialization Data:    0

          WID		EBR Instance
          ---		------------
          0b0000000011	LCDCharMap_inst/LCDCharMap_0_0_0
          0b0000000100	STRING_TABLE_INST/EXT_ROM_INST/pmi_romXhmenusdn8101024_0_0_0
          0b0000000101
         lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_1_1_0
          0b0000000110
         lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_0_0_3
          0b0000000111
         lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_0_1_2
          0b0000001000
         lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_1_0_1

    ASIC Components
    ---------------

    Instance Name: PowerCntr_inst/PCNTR_Inst0
             Type: PCNTR
    Instance Name: LCDCharMap_inst/LCDCharMap_0_0_0
             Type: DP8KC
    Instance Name: EFB_Inst/EFBInst_0
             Type: EFB
    Instance Name: STRING_TABLE_INST/EXT_ROM_INST/pmi_romXhmenusdn8101024_0_0_0
             Type: DP8KC
    Instance Name: lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_1_1_0
             Type: DP8KC
    Instance Name: lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_0_0_3
             Type: DP8KC
    Instance Name: lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_0_1_2
             Type: DP8KC
    Instance Name: lm8_inst/u1_isp8/u1_isp8_prom/pmi_romXhprom_initadn18112048_1_0_1
             Type: DP8KC
    Instance Name: clkselect_wb_inst/OSCH_inst

             Type: OSCH
    Instance Name: BankController_inst/InRD_2
             Type: BCINRD

    GSR Usage
    ---------

    GSR Component:
       The local reset signal 'wb_rst' of the design has been inferred as Global Set
            Reset (GSR). The reset signal used for GSR control is 'wb_rst'.

    GSR Property:
       The design components with GSR property set to ENABLED will respond to global
            set reset while the components with GSR property set to DISABLED will
            not.

    Components on inferred reset domain with GSR Property disabled
    --------------------------------------------------------------

    These components have the GSR property set to DISABLED and are on the inferred
         reset domain. The components will respond to the reset signal 'wb_rst' via
         the local reset on the component and not the GSR component.

    Type and number of components of the type:
       Register = 9
       DP8KC = 1, EFB = 1

    Type and instance name of component:
       Register : lm8_wb_inst/lm8_ext_io_din[7]
       Register : lm8_wb_inst/lm8_ext_io_din[6]
       Register : lm8_wb_inst/lm8_ext_io_din[5]
       Register : lm8_wb_inst/lm8_ext_io_din[4]
       Register : lm8_wb_inst/lm8_ext_io_din[3]
       Register : lm8_wb_inst/lm8_ext_io_din[2]
       Register : lm8_wb_inst/lm8_ext_io_din[1]
       Register : lm8_wb_inst/lm8_ext_io_din[0]
       Register : lm8_wb_inst/ack_reg
       DP8KC : STRING_TABLE_INST/EXT_ROM_INST/pmi_romXhmenusdn8101024_0_0_0
       EFB : EFB_Inst/EFBInst_0

    PGROUP Utilization

    PGROUP "RingOSC_group":
       Logic contained: 3 SLICEs, 1 PFUs
       Bounded Area:    4 PFUs (DEVSIZE) (ANCHORED)

    Run Time and Memory Usage
    -------------------------

       Total CPU Time: 1 secs
       Total REAL Time: 2 secs
       Peak Memory Usage: 39 MB

    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995
         AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent
         Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems
         All rights reserved.
    Copyright (c) 2002-2012 Lattice Semiconductor
         Corporation,  All rights reserved.