    PAD Specification File
    ***************************

    PART TYPE:        LCMXO2-1200ZE
    Performance Grade:      3
    PACKAGE:          CSBGA132
    Package Status:                     Final          Version 1.33

    Tue Jul 24 16:14:04 2012

    Pinout by Port Name:
    +-------------------+----------+---------------+-------+-----------+----------------------------------------+----------------------------------------------------------+
    | Port Name         | Pin/Bank | Buffer Type   | Site  | PG Enable | BC Enable                              | Properties                                               |
    +-------------------+----------+---------------+-------+-----------+----------------------------------------+----------------------------------------------------------+
    | EnAMP             | P2/2     | LVCMOS25_OUT  | PB4A  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | EnTempSPI         | N2/2     | LVCMOS25_OUT  | PB4B  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | I2CAlert          | B7/0     | LVCMOS25_OUT  | PT12B |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | Icc_analog_cmp_p  | P8/2     | LVDS25_IN     | PB15A |           | BankController_inst/InRD_2_INRDENO_SIG |                                                          |
    | Icc_analog_out    | P9/2     | LVCMOS25_OUT  | PB15C |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | Icco_analog_cmp_p | M9/2     | LVDS25_IN     | PB18A |           | BankController_inst/InRD_2_INRDENO_SIG |                                                          |
    | Icco_analog_out   | N9/2     | LVCMOS25_OUT  | PB15D |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_10            | K14/1    | LVCMOS25_OUT  | PR9B  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_11            | L14/1    | LVCMOS25_OUT  | PR9C  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_12            | M13/1    | LVCMOS25_OUT  | PR9D  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_5             | J12/1    | LVCMOS25_OUT  | PR8A  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_6             | J14/1    | LVCMOS25_OUT  | PR8B  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_7             | J13/1    | LVCMOS25_OUT  | PR8C  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_8             | K12/1    | LVCMOS25_OUT  | PR8D  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_9             | K13/1    | LVCMOS25_OUT  | PR9A  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_COM0          | B14/1    | LVCMOS25_OUT  | PR2A  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_COM1          | C13/1    | LVCMOS25_OUT  | PR2B  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_COM2          | C14/1    | LVCMOS25_OUT  | PR2C  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | LCD_COM3          | D12/1    | LVCMOS25_OUT  | PR2D  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    | PushBn            | N3/2     | LVCMOS25_IN   | PB6A  |           |                                        | CLAMP:ON HYSTERESIS:SMALL                                |
    | cap_btn1          | M10/2    | LVCMOS25_BIDI | PB18C |           |                                        | DRIVE:8mA PULL:DOWN CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
    | cap_btn2          | P11/2    | LVCMOS25_BIDI | PB18D |           |                                        | DRIVE:8mA PULL:DOWN CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
    | cap_btn3          | M11/2    | LVCMOS25_BIDI | PB20A |           |                                        | DRIVE:8mA PULL:DOWN CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
    | cap_btn4          | P12/2    | LVCMOS25_BIDI | PB20B |           |                                        | DRIVE:8mA PULL:DOWN CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW  |
    | clk_USB           | A7/0     | LVCMOS25_IN   | PT12A |           |                                        | CLAMP:ON HYSTERESIS:SMALL                                |
    | rst               | K1/3     | LVCMOS25_IN   | PL9A  |           |                                        | CLAMP:ON HYSTERESIS:SMALL                                |
    | scl               | C8/0     | LVCMOS25_BIDI | PT12C |           |                                        | DRIVE:8mA CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW            |
    | sda               | B8/0     | LVCMOS25_BIDI | PT12D |           |                                        | DRIVE:8mA CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW            |
    | spi_csn           | P3/2     | LVCMOS25_OUT  | PB4C  |           |                                        | DRIVE:8mA PULL:UP SLEW:SLOW                              |
    | spi_miso          | N4/2     | LVCMOS25_BIDI | PB6D  |           |                                        | DRIVE:8mA CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW            |
    | spi_mosi          | P13/2    | LVCMOS25_BIDI | PB20D |           |                                        | DRIVE:8mA CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW            |
    | spi_sclk          | M4/2     | LVCMOS25_BIDI | PB6C  |           |                                        | DRIVE:8mA CLAMP:ON HYSTERESIS:SMALL SLEW:SLOW            |
    | uart_rx           | E1/3     | LVCMOS25_IN   | PL3C  |           |                                        | CLAMP:ON HYSTERESIS:SMALL                                |
    | uart_tx           | E2/3     | LVCMOS25_OUT  | PL3D  |           |                                        | DRIVE:8mA SLEW:SLOW                                      |
    +-------------------+----------+---------------+-------+-----------+----------------------------------------+----------------------------------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 0    | 2.5V  |
    | 1    | 2.5V  |
    | 2    | 2.5V  |
    | 3    | 2.5V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------+-----------------------+------------+---------------+-------+-------------------------------------+-----------+----------------------------------------+
    | Pin/Bank | Pin Info              | Preference | Buffer Type   | Site  | Dual Function                       | PG Enable | BC Enable                              |
    +----------+-----------------------+------------+---------------+-------+-------------------------------------+-----------+----------------------------------------+
    | A2/0     |     unused, PULL:DOWN |            |               | PT9A  | L_GPLLT_MFGOUT2                     |           |                                        |
    | A3/0     |     unused, PULL:DOWN |            |               | PT10A | L_GPLLT_MFGOUT1                     |           |                                        |
    | A4/0     | Reserved: sysCONFIG   |            |               | PT10C | TDO                                 |           |                                        |
    | A6/0     | Reserved: sysCONFIG   |            |               | PT11D | TMS                                 |           |                                        |
    | A7/0     | clk_USB               | LOCATED    | LVCMOS25_IN   | PT12A | PCLKT0_1                            |           |                                        |
    | A9/0     |     unused, PULL:DOWN |            |               | PT15B |                                     |           |                                        |
    | A10/0    |     unused, PULL:DOWN |            |               | PT16A |                                     |           |                                        |
    | A11/0    |     unused, PULL:DOWN |            |               | PT16C |                                     |           |                                        |
    | A12/0    |     unused, PULL:DOWN |            |               | PT17B |                                     |           |                                        |
    | A13/0    |     unused, PULL:DOWN |            |               | PT17D | DONE                                |           |                                        |
    | B1/3     |     unused, PULL:DOWN |            |               | PL2A  | L_GPLLT_FB                          |           |                                        |
    | B2/3     |     unused, PULL:DOWN |            |               | PL2B  | L_GPLLC_FB                          |           |                                        |
    | B3/0     |     unused, PULL:DOWN |            |               | PT9B  | L_GPLLC_MFGOUT2                     |           |                                        |
    | B4/0     | Reserved: sysCONFIG   |            |               | PT10D | TDI/MD7                             |           |                                        |
    | B5/0     |     unused, PULL:DOWN |            |               | PT11A |                                     |           |                                        |
    | B6/0     | Reserved: sysCONFIG   |            |               | PT11C | TCK/TEST_CLK                        |           |                                        |
    | B7/0     | I2CAlert              | LOCATED    | LVCMOS25_OUT  | PT12B | PCLKC0_1                            |           |                                        |
    | B8/0     | sda                   | LOCATED    | LVCMOS25_BIDI | PT12D | SDA/IO3/MD3/ATB_FORCE/PCLKC0_0/TDOT |           |                                        |
    | B9/0     |     unused, PULL:DOWN |            |               | PT15C | JTAGENB/MD6/TDIR                    |           |                                        |
    | B12/0    |     unused, PULL:DOWN |            |               | PT16D |                                     |           |                                        |
    | B13/0    |     unused, PULL:DOWN |            |               | PT17C | INITN                               |           |                                        |
    | B14/1    | LCD_COM0              | LOCATED    | LVCMOS25_OUT  | PR2A  | DQ0                                 |           |                                        |
    | C1/3     |     unused, PULL:DOWN |            |               | PL2C  | L_GPLLT_IN                          |           |                                        |
    | C2/3     |     unused, PULL:DOWN |            |               | PL3A  | PCLKT3_2                            |           |                                        |
    | C3/3     |     unused, PULL:DOWN |            |               | PL2D  | L_GPLLC_IN                          |           |                                        |
    | C4/0     |     unused, PULL:DOWN |            |               | PT10B | L_GPLLC_MFGOUT1                     |           |                                        |
    | C6/0     |     unused, PULL:DOWN |            |               | PT11B |                                     |           |                                        |
    | C8/0     | scl                   | LOCATED    | LVCMOS25_BIDI | PT12C | SCL/IO2/MD2/ATB_SENSE/PCLKT0_0      |           |                                        |
    | C9/0     |     unused, PULL:DOWN |            |               | PT15A |                                     |           |                                        |
    | C10/0    |     unused, PULL:DOWN |            |               | PT15D | PROGRAMN                            |           |                                        |
    | C11/0    |     unused, PULL:DOWN |            |               | PT16B |                                     |           |                                        |
    | C12/0    |     unused, PULL:DOWN |            |               | PT17A |                                     |           |                                        |
    | C13/1    | LCD_COM1              | LOCATED    | LVCMOS25_OUT  | PR2B  | DQ0                                 |           |                                        |
    | C14/1    | LCD_COM2              | LOCATED    | LVCMOS25_OUT  | PR2C  | DQ0                                 |           |                                        |
    | D1/3     |     unused, PULL:DOWN |            |               | PL3B  | PCLKC3_2                            |           |                                        |
    | D12/1    | LCD_COM3              | LOCATED    | LVCMOS25_OUT  | PR2D  | DQ0                                 |           |                                        |
    | E1/3     | uart_rx               | LOCATED    | LVCMOS25_IN   | PL3C  |                                     |           |                                        |
    | E2/3     | uart_tx               | LOCATED    | LVCMOS25_OUT  | PL3D  |                                     |           |                                        |
    | E3/3     |     unused, PULL:DOWN |            |               | PL4A  |                                     |           |                                        |
    | E12/1    |     unused, PULL:DOWN |            |               | PR3A  | DQ0                                 |           |                                        |
    | E13/1    |     unused, PULL:DOWN |            |               | PR4A  | DQ0                                 |           |                                        |
    | E14/1    |     unused, PULL:DOWN |            |               | PR3B  | DQ0                                 |           |                                        |
    | F1/3     |     unused, PULL:DOWN |            |               | PL4C  |                                     |           |                                        |
    | F2/3     |     unused, PULL:DOWN |            |               | PL4B  |                                     |           |                                        |
    | F3/3     |     unused, PULL:DOWN |            |               | PL4D  |                                     |           |                                        |
    | F12/1    |     unused, PULL:DOWN |            |               | PR4B  | DQ0                                 |           |                                        |
    | F13/1    |     unused, PULL:DOWN |            |               | PR4C  | DQ0                                 |           |                                        |
    | F14/1    |     unused, PULL:DOWN |            |               | PR4D  | DQ0                                 |           |                                        |
    | G3/3     |     unused, PULL:DOWN |            |               | PL5A  | PCLKT3_1                            |           |                                        |
    | G12/1    |     unused, PULL:DOWN |            |               | PR5A  | DQS0                                |           |                                        |
    | G13/1    |     unused, PULL:DOWN |            |               | PR5C  | PCLKT1_0/DQ0                        |           |                                        |
    | G14/1    |     unused, PULL:DOWN |            |               | PR5B  | DQS0N                               |           |                                        |
    | H1/3     |     unused, PULL:DOWN |            |               | PL5C  |                                     |           |                                        |
    | H2/3     |     unused, PULL:DOWN |            |               | PL5B  | PCLKC3_1                            |           |                                        |
    | H3/3     |     unused, PULL:DOWN |            |               | PL5D  |                                     |           |                                        |
    | H12/1    |     unused, PULL:DOWN |            |               | PR5D  | PCLKC1_0/DQ0                        |           |                                        |
    | J1/3     |     unused, PULL:DOWN |            |               | PL8A  |                                     |           |                                        |
    | J2/3     |     unused, PULL:DOWN |            |               | PL8B  |                                     |           |                                        |
    | J3/3     |     unused, PULL:DOWN |            |               | PL8C  |                                     |           |                                        |
    | J12/1    | LCD_5                 | LOCATED    | LVCMOS25_OUT  | PR8A  | DQS1                                |           |                                        |
    | J13/1    | LCD_7                 | LOCATED    | LVCMOS25_OUT  | PR8C  | DQ1                                 |           |                                        |
    | J14/1    | LCD_6                 | LOCATED    | LVCMOS25_OUT  | PR8B  | DQS1N                               |           |                                        |
    | K1/3     | rst                   |            | LVCMOS25_IN   | PL9A  | PCLKT3_0                            |           |                                        |
    | K2/3     |     unused, PULL:DOWN |            |               | PL8D  |                                     |           |                                        |
    | K3/3     |     unused, PULL:DOWN |            |               | PL9B  | PCLKC3_0                            |           |                                        |
    | K12/1    | LCD_8                 | LOCATED    | LVCMOS25_OUT  | PR8D  | DQ1                                 |           |                                        |
    | K13/1    | LCD_9                 | LOCATED    | LVCMOS25_OUT  | PR9A  | DQ1                                 |           |                                        |
    | K14/1    | LCD_10                | LOCATED    | LVCMOS25_OUT  | PR9B  | DQ1                                 |           |                                        |
    | L3/3     |     unused, PULL:DOWN |            |               | PL10B |                                     |           |                                        |
    | L14/1    | LCD_11                | LOCATED    | LVCMOS25_OUT  | PR9C  | DQ1                                 |           |                                        |
    | M1/3     |     unused, PULL:DOWN |            |               | PL10C |                                     |           |                                        |
    | M2/3     |     unused, PULL:DOWN |            |               | PL10D |                                     |           |                                        |
    | M3/2     |     unused, PULL:DOWN |            |               | PB4D  |                                     |           |                                        |
    | M4/2     | spi_sclk              | LOCATED    | LVCMOS25_BIDI | PB6C  | MCLK/CCLK                           |           |                                        |
    | M5/2     |     unused, PULL:DOWN |            |               | PB9D  |                                     |           |                                        |
    | M7/2     |     unused, PULL:DOWN |            |               | PB11A | PCLKT2_1/INTEST_OVER                |           |                                        |
    | M8/2     | Icc_analog_cmp_n      |            | LVDS25_IN     | PB15B |                                     |           |                                        |
    | M9/2     | Icco_analog_cmp_p     | LOCATED    | LVDS25_IN     | PB18A |                                     |           | BankController_inst/InRD_2_INRDENO_SIG |
    | M10/2    | cap_btn1              | LOCATED    | LVCMOS25_BIDI | PB18C |                                     |           |                                        |
    | M11/2    | cap_btn3              | LOCATED    | LVCMOS25_BIDI | PB20A |                                     |           |                                        |
    | M12/1    |     unused, PULL:DOWN |            |               | PR10A | DQ1                                 |           |                                        |
    | M13/1    | LCD_12                | LOCATED    | LVCMOS25_OUT  | PR9D  | DQ1                                 |           |                                        |
    | M14/1    |     unused, PULL:DOWN |            |               | PR10B | DQ1                                 |           |                                        |
    | N2/2     | EnTempSPI             | LOCATED    | LVCMOS25_OUT  | PB4B  |                                     |           |                                        |
    | N3/2     | PushBn                | LOCATED    | LVCMOS25_IN   | PB6A  |                                     |           |                                        |
    | N4/2     | spi_miso              | LOCATED    | LVCMOS25_BIDI | PB6D  | SO/SPISO/IO1/MD1/TDIL               |           |                                        |
    | N5/2     |     unused, PULL:DOWN |            |               | PB9C  |                                     |           |                                        |
    | N6/2     |     unused, PULL:DOWN |            |               | PB9A  | PCLKT2_0/INTEST_OVER                |           |                                        |
    | N7/2     |     unused, PULL:DOWN |            |               | PB11D |                                     |           |                                        |
    | N8/2     |     unused, PULL:DOWN |            |               | PB11B | PCLKC2_1                            |           |                                        |
    | N9/2     | Icco_analog_out       | LOCATED    | LVCMOS25_OUT  | PB15D |                                     |           |                                        |
    | N10/2    | Icco_analog_cmp_n     |            | LVDS25_IN     | PB18B |                                     |           |                                        |
    | N12/2    | Reserved: sysCONFIG   |            | LVCMOS25_IN   | PB20C | SN/MD5/SCAN_SHFT_ENB/TDIB           |           |                                        |
    | N13/1    |     unused, PULL:DOWN |            |               | PR10C | DQ1                                 |           |                                        |
    | N14/1    |     unused, PULL:DOWN |            |               | PR10D | DQ1                                 |           |                                        |
    | P2/2     | EnAMP                 | LOCATED    | LVCMOS25_OUT  | PB4A  |                                     |           |                                        |
    | P3/2     | spi_csn               | LOCATED    | LVCMOS25_OUT  | PB4C  | CSSPIN/MD4/TDOB                     |           |                                        |
    | P4/2     |     unused, PULL:DOWN |            |               | PB6B  |                                     |           |                                        |
    | P6/2     |     unused, PULL:DOWN |            |               | PB9B  | PCLKC2_0                            |           |                                        |
    | P7/2     |     unused, PULL:DOWN |            |               | PB11C |                                     |           |                                        |
    | P8/2     | Icc_analog_cmp_p      | LOCATED    | LVDS25_IN     | PB15A |                                     |           | BankController_inst/InRD_2_INRDENO_SIG |
    | P9/2     | Icc_analog_out        | LOCATED    | LVCMOS25_OUT  | PB15C |                                     |           |                                        |
    | P11/2    | cap_btn2              | LOCATED    | LVCMOS25_BIDI | PB18D |                                     |           |                                        |
    | P12/2    | cap_btn4              | LOCATED    | LVCMOS25_BIDI | PB20B |                                     |           |                                        |
    | P13/2    | spi_mosi              | LOCATED    | LVCMOS25_BIDI | PB20D | SI/SISPI/IO0/MD0/TDOR               |           |                                        |
    | PL10A/3  |     unused, PULL:DOWN |            |               | PL10A |                                     |           |                                        |
    | PT9C/0   |     unused, PULL:DOWN |            |               | PT9C  |                                     |           |                                        |
    | PT9D/0   |     unused, PULL:DOWN |            |               | PT9D  |                                     |           |                                        |
    +----------+-----------------------+------------+---------------+-------+-------------------------------------+-----------+----------------------------------------+

    sysCONFIG Pins:
    +----------+-------------------------------------+-----------------------+----------+---------------+-------------------+
    | Pad Name | sysCONFIG Pin Name                  | sysCONFIG Settings    | Pin/Bank | Buffer Type   | Config Pull Mode  |
    +----------+-------------------------------------+-----------------------+----------+---------------+-------------------+
    | PT12D    | SDA/IO3/MD3/ATB_FORCE/PCLKC0_0/TDOT | I2C_PORT=ENABLE       | B8/0     | LVCMOS25_BIDI | NO pull up/down   |
    | PT12C    | SCL/IO2/MD2/ATB_SENSE/PCLKT0_0      | I2C_PORT=ENABLE       | C8/0     | LVCMOS25_BIDI | NO pull up/down   |
    | PT11D    | TMS                                 | JTAG_PORT=ENABLE      | A6/0     |               | PULLUP            |
    | PT11C    | TCK/TEST_CLK                        | JTAG_PORT=ENABLE      | B6/0     |               | NO pull up/down   |
    | PT10D    | TDI/MD7                             | JTAG_PORT=ENABLE      | B4/0     |               | PULLUP            |
    | PT10C    | TDO                                 | JTAG_PORT=ENABLE      | A4/0     |               | PULLUP            |
    | PB6C     | MCLK/CCLK                           | SLAVE_SPI_PORT=ENABLE | M4/2     | LVCMOS25_BIDI | NO pull up/down   |
    | PB6D     | SO/SPISO/IO1/MD1/TDIL               | SLAVE_SPI_PORT=ENABLE | N4/2     | LVCMOS25_BIDI | NO pull up/down   |
    | PB20C    | SN/MD5/SCAN_SHFT_ENB/TDIB           | SLAVE_SPI_PORT=ENABLE | N12/2    | LVCMOS25_IN   | PULLUP            |
    | PB20D    | SI/SISPI/IO0/MD0/TDOR               | SLAVE_SPI_PORT=ENABLE | P13/2    | LVCMOS25_BIDI | NO pull up/down   |
    +----------+-------------------------------------+-----------------------+----------+---------------+-------------------+

    Locate Preferences for each Pin:

    LOCATE  COMP  "EnAMP"  SITE  "P2";
    LOCATE  COMP  "EnTempSPI"  SITE  "N2";
    LOCATE  COMP  "I2CAlert"  SITE  "B7";
    LOCATE  COMP  "Icc_analog_cmp_p"  SITE  "P8";
    LOCATE  COMP  "Icc_analog_out"  SITE  "P9";
    LOCATE  COMP  "Icco_analog_cmp_p"  SITE  "M9";
    LOCATE  COMP  "Icco_analog_out"  SITE  "N9";
    LOCATE  COMP  "LCD_10"  SITE  "K14";
    LOCATE  COMP  "LCD_11"  SITE  "L14";
    LOCATE  COMP  "LCD_12"  SITE  "M13";
    LOCATE  COMP  "LCD_5"  SITE  "J12";
    LOCATE  COMP  "LCD_6"  SITE  "J14";
    LOCATE  COMP  "LCD_7"  SITE  "J13";
    LOCATE  COMP  "LCD_8"  SITE  "K12";
    LOCATE  COMP  "LCD_9"  SITE  "K13";
    LOCATE  COMP  "LCD_COM0"  SITE  "B14";
    LOCATE  COMP  "LCD_COM1"  SITE  "C13";
    LOCATE  COMP  "LCD_COM2"  SITE  "C14";
    LOCATE  COMP  "LCD_COM3"  SITE  "D12";
    LOCATE  COMP  "PushBn"  SITE  "N3";
    LOCATE  COMP  "cap_btn1"  SITE  "M10";
    LOCATE  COMP  "cap_btn2"  SITE  "P11";
    LOCATE  COMP  "cap_btn3"  SITE  "M11";
    LOCATE  COMP  "cap_btn4"  SITE  "P12";
    LOCATE  COMP  "clk_USB"  SITE  "A7";
    LOCATE  COMP  "rst"  SITE  "K1";
    LOCATE  COMP  "scl"  SITE  "C8";
    LOCATE  COMP  "sda"  SITE  "B8";
    LOCATE  COMP  "spi_csn"  SITE  "P3";
    LOCATE  COMP  "spi_miso"  SITE  "N4";
    LOCATE  COMP  "spi_mosi"  SITE  "P13";
    LOCATE  COMP  "spi_sclk"  SITE  "M4";
    LOCATE  COMP  "uart_rx"  SITE  "E1";
    LOCATE  COMP  "uart_tx"  SITE  "E2";

    PAR: Place And Route Diamond Version 2.0.0.154.
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2012 Lattice Semiconductor Corporation,  All rights reserved.
    Tue Jul 24 16:14:04 2012