    BITGEN: Bitstream Generator Diamond Version 2.0.0.154
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2012 Lattice Semiconductor Corporation,  All rights reserved.

    Command: bitgen -g RamCfg:Reset -path C:/asdf/MachXO2 Pico Demo from Website/doc41117x92/Demo_MachXO2_Pico_Environment_Scanning/project -w -jedec Environment_Scanning_impl1.ncd Environment_Scanning_impl1.prf

    Loading design for application Bitgen from file Environment_Scanning_impl1.ncd.
    Design name: Environment_Scanning
    NCD version: 3.2
    Vendor:      LATTICE
    Device:      LCMXO2-1200ZE
    Package:     CSBGA132
    Performance: 3
    Loading device for application Bitgen from file 'xo2c1200.nph' in environment: C:/Diamond/diamond/2.0/ispfpga.
    Package Status:                     Final          Version 1.33
    Performance Hardware Data Status:   Final          Version 22.4

    Running DRC.
    INFO: Design contains pre-loadable EBR during configuration that has a requirement: Since the GSR is disabled for the EBR, make sure write enable and chip enable are inactive during wake-up, so that the pre-loaded initialization values will not be corrupted during wake-up state.
    INFO: Design contains EBR with ASYNC Reset Mode that has a limitation: The use of the EBR block asynchronous reset requires that certain timing be met between the clock and the reset within the memory block. See the device specific datasheet for additional details.
    DRC detected 0 errors and 0 warnings.
    Reading Preference File from Environment_Scanning_impl1.prf...

    Preference Summary:

    +---------------------------------+---------------------------------+
    |  Preference                     |  Current Setting                |
    +---------------------------------+---------------------------------+
    |                         RamCfg  |                        Reset**  |
    +---------------------------------+---------------------------------+
    |                     MCCLK_FREQ  |                         2.08**  |
    +---------------------------------+---------------------------------+
    |                  CONFIG_SECURE  |                          OFF**  |
    +---------------------------------+---------------------------------+
    |                      JTAG_PORT  |                       ENABLE**  |
    +---------------------------------+---------------------------------+
    |                       SDM_PORT  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |                 SLAVE_SPI_PORT  |                         ENABLE  |
    +---------------------------------+---------------------------------+
    |                MASTER_SPI_PORT  |                       EFB_USER  |
    +---------------------------------+---------------------------------+
    |                       I2C_PORT  |                         ENABLE  |
    +---------------------------------+---------------------------------+
    |        MUX_CONFIGURATION_PORTS  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |             GENERATE_BITSTREAM  |                         ENABLE  |
    +---------------------------------+---------------------------------+
    |                  CONFIGURATION  |                          CFG**  |
    +---------------------------------+---------------------------------+
    |                COMPRESS_CONFIG  |                           ON**  |
    +---------------------------------+---------------------------------+
    |                        MY_ASSP  |                          OFF**  |
    +---------------------------------+---------------------------------+
    |               ONE_TIME_PROGRAM  |                          OFF**  |
    +---------------------------------+---------------------------------+
    |                 ENABLE_TRANSFR  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
    |                  SHAREDEBRINIT  |                      DISABLE**  |
    +---------------------------------+---------------------------------+
     *  Default setting.
     ** The specified setting matches the default setting.

    Creating bit map...

    Bitstream Status:   Final           Version 1.82

    ===========
    UFM Summary
    ===========
    UFM Size:        511 Pages (128*511 Bits)
    UFM Utilization: General Purpose Flash Memory

    Available General Purpose Flash Memory:  511 Pages (Page 0 to Page 510)
    Initialized UFM Pages:                     0 Page

    Saving bit stream in Environment_Scanning_impl1.bit.
    Saving JEDEC in Environment_Scanning_impl1.jed.