@N|Running in 32-bit mode
@N: CG334 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_bit_ctrl.v":161:12:161:24|Read directive translate_off 
@N: CG333 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_bit_ctrl.v":163:12:163:23|Read directive translate_on 
@N: CG346 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_bit_ctrl.v":394:38:394:46|Read full_case directive 
@N: CG347 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_bit_ctrl.v":394:48:394:60|Read parallel_case directive 
@N: CG346 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_bit_ctrl.v":398:40:398:48|Read full_case directive 
@N: CG347 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_bit_ctrl.v":398:50:398:62|Read parallel_case directive 
@N: CG334 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_byte_ctrl.v":106:12:106:24|Read directive translate_off 
@N: CG333 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_byte_ctrl.v":108:12:108:23|Read directive translate_on 
@N: CG346 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_byte_ctrl.v":275:34:275:42|Read full_case directive 
@N: CG347 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_byte_ctrl.v":275:44:275:56|Read parallel_case directive 
@N: CG334 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_wb_top.v":110:12:110:24|Read directive translate_off 
@N: CG333 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1046\source\i2c_master_wb_top.v":112:12:112:23|Read directive translate_on 
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":557:7:557:11|Synthesizing module ILVDS
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":1705:7:1705:12|Synthesizing module BCINRD
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\source\IPexpress\BankController.v":8:7:8:20|Synthesizing module BankController
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\reset_gen.v":46:7:46:15|Synthesizing module reset_gen
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\led_sw_wb.v":45:7:45:15|Synthesizing module lcd_sw_wb
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\USBorBatt_wb.v":46:7:46:18|Synthesizing module USBorBatt_wb
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\ringosc.v":46:7:46:13|Synthesizing module RingOSC
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":1793:7:1793:10|Synthesizing module OSCH
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\oscclkclean.v":46:7:46:17|Synthesizing module oscclkclean
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\clk_switch.v":44:7:44:16|Synthesizing module clk_switch
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\clksource_wb.v":46:7:46:18|Synthesizing module clkselect_wb
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1043\source\lm8_wb.v":47:7:47:12|Synthesizing module lm8_wb
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_idec.v":40:7:40:15|Synthesizing module isp8_idec
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_alu.v":135:7:135:16|Synthesizing module pmi_addsub
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_alu.v":41:7:41:14|Synthesizing module isp8_alu
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\lm8_top.v":142:7:142:27|Synthesizing module pmi_distributed_spram
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_flow_cntl.v":41:7:41:20|Synthesizing module isp8_flow_cntl
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_flow_cntl.v":229:28:229:36|Removing redundant assignment
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_flow_cntl.v":358:23:358:29|Removing redundant assignment
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_flow_cntl.v":375:28:375:39|Removing redundant assignment
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_io_cntl.v":39:8:39:19|Synthesizing module isp8_io_cntl
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_core.v":513:7:513:13|Synthesizing module pmi_rom
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_core.v":42:7:42:15|Synthesizing module isp8_core
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_core.v":337:28:337:36|Removing redundant assignment
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_core.v":349:28:349:36|Removing redundant assignment
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_core.v":488:7:488:27|Synthesizing module pmi_distributed_dpram
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\lm8_top.v":142:7:142:27|Synthesizing module pmi_distributed_spram
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\lm8_top.v":46:7:46:10|Synthesizing module isp8
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\intface.v":51:7:51:13|Synthesizing module intface
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\rxcver.v":49:7:49:12|Synthesizing module rxcver
@N: CL177 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\rxcver.v":426:3:426:8|Sharing sequential element sin_d0_delay.
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\txmitt.v":48:7:48:12|Synthesizing module txmitt
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\modem.v":49:7:49:11|Synthesizing module modem
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\uart_core.v":52:7:52:15|Synthesizing module uart_core
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1066\source\verilog\box_ave.v":66:7:66:13|Synthesizing module box_ave
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1066\source\verilog\sigmadelta_adc.v":62:7:62:20|Synthesizing module sigmadelta_adc
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1066\source\verilog\adc_top.v":62:7:62:13|Synthesizing module ADC_top
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\adc_wb.v":45:7:45:12|Synthesizing module adc_wb
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\adc_wb.v":73:16:73:24|Removing redundant assignment
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\latticemico8_v3_1_verilog\source\isp8_core.v":513:7:513:13|Synthesizing module pmi_rom
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\rom_ebr_wb.v":45:7:45:16|Synthesizing module rom_ebr_wb
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":1120:7:1120:9|Synthesizing module VHI
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":82:7:82:8|Synthesizing module BB
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":1124:7:1124:9|Synthesizing module VLO
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":1800:7:1800:9|Synthesizing module EFB
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\source\IPexpress\EFB_Module.v":8:7:8:16|Synthesizing module EFB_Module
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\capsense.v":54:7:54:14|Synthesizing module capsense
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\capsense.v":209:17:209:24|Removing redundant assignment
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\capsense.v":219:17:219:24|Removing redundant assignment
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\capsense.v":229:17:229:24|Removing redundant assignment
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\capsense.v":239:17:239:24|Removing redundant assignment
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\lcdencoding4to1com.v":45:7:45:24|Synthesizing module LCDEncoding4to1com
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\pwm.v":45:7:45:9|Synthesizing module PWM
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\LCDEncoding4to1.v":45:7:45:21|Synthesizing module LCDEncoding4to1
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\lcd4digit.v":43:7:43:15|Synthesizing module LCD4Digit
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":1291:7:1291:11|Synthesizing module DP8KC
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\source\IPexpress\LCDCharMap.v":8:7:8:16|Synthesizing module LCDCharMap
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\debounce.v":44:7:44:26|Synthesizing module PushButton_Debouncer
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\debounce.v":74:13:74:18|Removing redundant assignment
@N: CG364 :"C:\Diamond\diamond\2.0\cae_library\synthesis\verilog\machxo2.v":1694:7:1694:11|Synthesizing module PCNTR
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\source\PowerCntr.v":8:7:8:15|Synthesizing module PowerCntr
@N: CG364 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\Environment_Scanning.v":46:7:46:26|Synthesizing module Environment_Scanning
@N: CG179 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\Environment_Scanning.v":753:19:753:30|Removing redundant assignment
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\Environment_Scanning.v":878:1:878:6|Trying to extract state machine for register state
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\Environment_Scanning.v":749:1:749:6|Trying to extract state machine for register lcdstate
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\LCDEncoding4to1.v":110:1:110:6|Trying to extract state machine for register state
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\pwm.v":101:1:101:6|Trying to extract state machine for register state
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\source\lcdencoding4to1com.v":100:1:100:6|Trying to extract state machine for register state
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\modem.v":99:2:99:7|Trying to extract state machine for register msr_reg
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\txmitt.v":275:3:275:8|Trying to extract state machine for register genblk2.genblk1.tx_state
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\rxcver.v":269:3:269:8|Trying to extract state machine for register cs_state
@N: CL201 :"C:\asdf\MachXO2 Pico Demo from Website\doc41117x92\Demo_MachXO2_Pico_Environment_Scanning\project\..\rd1042\source\intface.v":579:3:579:8|Trying to extract state machine for register genblk13.cs_state

