    PAD Specification File
    ***************************

    PART TYPE:        LFMXO4-110HC
    Performance Grade:      5
    PACKAGE:          BBG484
    Package Status:                     Advanced       Version 2

    Sat Nov 15 12:18:41 2025

    Pinout by Port Name:
    +-----------+----------+--------------+-------+-----------------------------------------------------------------------------------------------------------------------------+
    | Port Name | Pin/Bank | Buffer Type  | Site  | Properties                                                                                                                  |
    +-----------+----------+--------------+-------+-----------------------------------------------------------------------------------------------------------------------------+
    | led[0]    | F4/5     | LVCMOS25_OUT | PL5D  | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | led[1]    | G4/5     | LVCMOS25_OUT | PL6D  | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | led[2]    | G3/5     | LVCMOS25_OUT | PL6C  | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | led[3]    | G1/5     | LVCMOS25_OUT | PL7B  | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | led[4]    | H2/5     | LVCMOS25_OUT | PL10A | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | led[5]    | H1/5     | LVCMOS25_OUT | PL10B | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | led[6]    | J2/5     | LVCMOS25_OUT | PL12A | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | led[7]    | J1/5     | LVCMOS25_OUT | PL12B | DRIVE:8mA SLEWRATE:SLOW HYSTERESIS:NA OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:OFF  |
    | rstn      | D3/5     | LVCMOS25_IN  | PL2A  | DRIVE: SLEWRATE:NA HYSTERESIS:SMALL OPENDRAIN:OFF IO_TYPE:LVCMOS25 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON     |
    +-----------+----------+--------------+-------+-----------------------------------------------------------------------------------------------------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 5    | 2.5V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------+-----------------------+------------+--------------+-------+-------------------------------------+
    | Pin/Bank | Pin Info              | Preference | Buffer Type  | Site  | Dual Function                       |
    +----------+-----------------------+------------+--------------+-------+-------------------------------------+
    | A2/0     |     unused, PULL:DOWN |            |              | PT9B  | L_GPLLC_MFGOUT2                     |
    | A3/0     |     unused, PULL:DOWN |            |              | PT10B |                                     |
    | A4/0     |     unused, PULL:DOWN |            |              | PT11B | L_GPLLC_MFGOUT1                     |
    | A5/0     |     unused, PULL:DOWN |            |              | PT12B |                                     |
    | A6/0     |     unused, PULL:DOWN |            |              | PT13B |                                     |
    | A7/0     |     unused, PULL:DOWN |            |              | PT14B |                                     |
    | A8/0     |     unused, PULL:DOWN |            |              | PT20B |                                     |
    | A9/0     |     unused, PULL:DOWN |            |              | PT21B |                                     |
    | A10/0    |     unused, PULL:DOWN |            |              | PT23B | PCLKC0_1                            |
    | A11/0    |     unused, PULL:DOWN |            |              | PT24B |                                     |
    | A12/0    |     unused, PULL:DOWN |            |              | PT27D | SDA/IO3/MD3/ATB_FORCE/PCLKC0_0/TDOT |
    | A13/0    |     unused, PULL:DOWN |            |              | PT29A |                                     |
    | A14/0    |     unused, PULL:DOWN |            |              | PT30A |                                     |
    | A15/0    |     unused, PULL:DOWN |            |              | PT38A |                                     |
    | A16/0    |     unused, PULL:DOWN |            |              | PT39A |                                     |
    | A17/0    |     unused, PULL:DOWN |            |              | PT40A |                                     |
    | A18/0    |     unused, PULL:DOWN |            |              | PT41A |                                     |
    | A19/0    |     unused, PULL:DOWN |            |              | PT42A |                                     |
    | A21/0    |     unused, PULL:DOWN |            |              | PT44A | R_GPLLT_MFGOUT1                     |
    | AA1/3    |     unused, PULL:DOWN |            |              | PL29B |                                     |
    | AA2/2    |     unused, PULL:DOWN |            |              | PB5A  |                                     |
    | AA3/2    |     unused, PULL:DOWN |            |              | PB7A  | CSSPIN/MD4/TDOB                     |
    | AA4/2    |     unused, PULL:DOWN |            |              | PB8A  |                                     |
    | AA5/2    |     unused, PULL:DOWN |            |              | PB10A |                                     |
    | AA6/2    |     unused, PULL:DOWN |            |              | PB11A |                                     |
    | AA7/2    |     unused, PULL:DOWN |            |              | PB13A |                                     |
    | AA8/2    |     unused, PULL:DOWN |            |              | PB18A |                                     |
    | AA9/2    |     unused, PULL:DOWN |            |              | PB19A |                                     |
    | AA10/2   |     unused, PULL:DOWN |            |              | PB22A | PCLKT2_0/INTEST_OVER                |
    | AA11/2   |     unused, PULL:DOWN |            |              | PB24A |                                     |
    | AA12/2   |     unused, PULL:DOWN |            |              | PB29B | PCLKC2_1                            |
    | AA13/2   |     unused, PULL:DOWN |            |              | PB30B |                                     |
    | AA14/2   |     unused, PULL:DOWN |            |              | PB33B |                                     |
    | AA15/2   |     unused, PULL:DOWN |            |              | PB35B |                                     |
    | AA16/2   |     unused, PULL:DOWN |            |              | PB38B |                                     |
    | AA17/2   |     unused, PULL:DOWN |            |              | PB40B |                                     |
    | AA18/2   |     unused, PULL:DOWN |            |              | PB41B |                                     |
    | AA19/2   |     unused, PULL:DOWN |            |              | PB43B |                                     |
    | AA20/2   |     unused, PULL:DOWN |            |              | PB44B |                                     |
    | AA21/2   |     unused, PULL:DOWN |            |              | PB46B | SI/SISPI/IO0/MD0/TDOR               |
    | AA22/1   |     unused, PULL:DOWN |            |              | PR29A | DQ1                                 |
    | AB2/2    |     unused, PULL:DOWN |            |              | PB5B  |                                     |
    | AB3/2    |     unused, PULL:DOWN |            |              | PB7B  |                                     |
    | AB4/2    |     unused, PULL:DOWN |            |              | PB8B  |                                     |
    | AB5/2    |     unused, PULL:DOWN |            |              | PB10B |                                     |
    | AB6/2    |     unused, PULL:DOWN |            |              | PB11B |                                     |
    | AB7/2    |     unused, PULL:DOWN |            |              | PB13B |                                     |
    | AB8/2    |     unused, PULL:DOWN |            |              | PB18B |                                     |
    | AB9/2    |     unused, PULL:DOWN |            |              | PB19B |                                     |
    | AB10/2   |     unused, PULL:DOWN |            |              | PB22B | PCLKC2_0                            |
    | AB11/2   |     unused, PULL:DOWN |            |              | PB24B |                                     |
    | AB12/2   |     unused, PULL:DOWN |            |              | PB29A | PCLKT2_1/INTEST_OVER                |
    | AB13/2   |     unused, PULL:DOWN |            |              | PB30A |                                     |
    | AB14/2   |     unused, PULL:DOWN |            |              | PB33A |                                     |
    | AB15/2   |     unused, PULL:DOWN |            |              | PB35A |                                     |
    | AB16/2   |     unused, PULL:DOWN |            |              | PB38A |                                     |
    | AB17/2   |     unused, PULL:DOWN |            |              | PB40A |                                     |
    | AB18/2   |     unused, PULL:DOWN |            |              | PB41A |                                     |
    | AB19/2   |     unused, PULL:DOWN |            |              | PB43A |                                     |
    | AB20/2   |     unused, PULL:DOWN |            |              | PB44A |                                     |
    | AB21/2   |     unused, PULL:DOWN |            |              | PB46A | SN/MD5/SCAN_SHFT_ENB/TDIB           |
    | B1/0     |     unused, PULL:DOWN |            |              | PT9A  | L_GPLLT_MFGOUT2                     |
    | B2/0     |     unused, PULL:DOWN |            |              | PT10A |                                     |
    | B4/0     |     unused, PULL:DOWN |            |              | PT12A |                                     |
    | B5/0     |     unused, PULL:DOWN |            |              | PT13A |                                     |
    | B6/0     |     unused, PULL:DOWN |            |              | PT14A |                                     |
    | B8/0     |     unused, PULL:DOWN |            |              | PT20A |                                     |
    | B9/0     |     unused, PULL:DOWN |            |              | PT21A |                                     |
    | B10/0    |     unused, PULL:DOWN |            |              | PT23A | PCLKT0_1                            |
    | B11/0    |     unused, PULL:DOWN |            |              | PT24A |                                     |
    | B12/0    |     unused, PULL:DOWN |            |              | PT27C | SCL/IO2/MD2/ATB_SENSE/PCLKT0_0      |
    | B13/0    |     unused, PULL:DOWN |            |              | PT29B |                                     |
    | B14/0    |     unused, PULL:DOWN |            |              | PT30B |                                     |
    | B15/0    |     unused, PULL:DOWN |            |              | PT38B |                                     |
    | B17/0    |     unused, PULL:DOWN |            |              | PT39B |                                     |
    | B18/0    |     unused, PULL:DOWN |            |              | PT40B |                                     |
    | B19/0    |     unused, PULL:DOWN |            |              | PT41B |                                     |
    | B20/0    |     unused, PULL:DOWN |            |              | PT42B |                                     |
    | B21/0    |     unused, PULL:DOWN |            |              | PT43B | R_GPLLC_MFGOUT2                     |
    | B22/0    |     unused, PULL:DOWN |            |              | PT44B | R_GPLLC_MFGOUT1                     |
    | C1/5     |     unused, PULL:DOWN |            |              | PL4A  | L_GPLLT_IN                          |
    | C3/0     |     unused, PULL:DOWN |            |              | PT10C |                                     |
    | C4/0     |     unused, PULL:DOWN |            |              | PT10D |                                     |
    | C5/0     |     unused, PULL:DOWN |            |              | PT12D |                                     |
    | C6/0     |     unused, PULL:DOWN |            |              | PT14C |                                     |
    | C8/0     |     unused, PULL:DOWN |            |              | PT15A |                                     |
    | C9/0     |     unused, PULL:DOWN |            |              | PT20C |                                     |
    | C10/0    | Reserved: sysCONFIG   |            |              | PT22D | TMS                                 |
    | C13/0    |     unused, PULL:DOWN |            |              | PT29C |                                     |
    | C14/0    |     unused, PULL:DOWN |            |              | PT30C |                                     |
    | C15/0    |     unused, PULL:DOWN |            |              | PT38C |                                     |
    | C17/0    |     unused, PULL:DOWN |            |              | PT39C |                                     |
    | C18/0    |     unused, PULL:DOWN |            |              | PT41C |                                     |
    | C19/0    |     unused, PULL:DOWN |            |              | PT43C |                                     |
    | C20/0    |     unused, PULL:DOWN |            |              | PT43D |                                     |
    | C21/1    |     unused, PULL:DOWN |            |              | PR2A  | R_GPLLT_FB/DQ0                      |
    | C22/1    |     unused, PULL:DOWN |            |              | PR2B  | R_GPLLC_FB/DQ0                      |
    | D1/5     |     unused, PULL:DOWN |            |              | PL5A  |                                     |
    | D2/5     |     unused, PULL:DOWN |            |              | PL4B  | L_GPLLC_IN                          |
    | D3/5     | rstn                  | LOCATED    | LVCMOS25_IN  | PL2A  |                                     |
    | D4/5     |     unused, PULL:DOWN |            |              | PL2B  |                                     |
    | D5/0     |     unused, PULL:DOWN |            |              | PT12C |                                     |
    | D6/0     |     unused, PULL:DOWN |            |              | PT13C |                                     |
    | D7/0     |     unused, PULL:DOWN |            |              | PT14D |                                     |
    | D8/0     |     unused, PULL:DOWN |            |              | PT15B |                                     |
    | D9/0     |     unused, PULL:DOWN |            |              | PT20D |                                     |
    | D10/0    | Reserved: sysCONFIG   |            |              | PT22C | TCK/TEST_CLK                        |
    | D11/0    |     unused, PULL:DOWN |            |              | PT24D |                                     |
    | D12/0    |     unused, PULL:DOWN |            |              | PT27A |                                     |
    | D13/0    |     unused, PULL:DOWN |            |              | PT29D |                                     |
    | D14/0    |     unused, PULL:DOWN |            |              | PT30D |                                     |
    | D15/0    |     unused, PULL:DOWN |            |              | PT38D |                                     |
    | D16/0    |     unused, PULL:DOWN |            |              | PT39D |                                     |
    | D17/0    |     unused, PULL:DOWN |            |              | PT40D |                                     |
    | D18/0    |     unused, PULL:DOWN |            |              | PT41D |                                     |
    | D19/1    |     unused, PULL:DOWN |            |              | PR3C  |                                     |
    | D20/1    |     unused, PULL:DOWN |            |              | PR3D  |                                     |
    | D21/1    |     unused, PULL:DOWN |            |              | PR3B  | R_GPLLC_IN/DQ0                      |
    | D22/1    |     unused, PULL:DOWN |            |              | PR3A  | R_GPLLT_IN/DQ0                      |
    | E1/5     |     unused, PULL:DOWN |            |              | PL6A  |                                     |
    | E2/5     |     unused, PULL:DOWN |            |              | PL5B  |                                     |
    | E3/5     |     unused, PULL:DOWN |            |              | PL5C  |                                     |
    | E4/5     |     unused, PULL:DOWN |            |              | PL3A  | L_GPLLT_FB                          |
    | E6/0     |     unused, PULL:DOWN |            |              | PT9C  |                                     |
    | E7/0     |     unused, PULL:DOWN |            |              | PT13D |                                     |
    | E8/0     | Reserved: sysCONFIG   |            |              | PT15C | TDO                                 |
    | E9/0     | Reserved: sysCONFIG   |            |              | PT15D | TDI/MD7                             |
    | E10/0    |     unused, PULL:DOWN |            |              | PT22B |                                     |
    | E11/0    |     unused, PULL:DOWN |            |              | PT24C |                                     |
    | E12/0    |     unused, PULL:DOWN |            |              | PT27B |                                     |
    | E13/0    |     unused, PULL:DOWN |            |              | PT28C |                                     |
    | E14/0    |     unused, PULL:DOWN |            |              | PT31C | JTAGENB/MD6/TDIR                    |
    | E15/0    |     unused, PULL:DOWN |            |              | PT31D | PROGRAMN                            |
    | E16/0    |     unused, PULL:DOWN |            |              | PT40C |                                     |
    | E17/0    |     unused, PULL:DOWN |            |              | PT44D | DONE                                |
    | E19/1    |     unused, PULL:DOWN |            |              | PR4C  |                                     |
    | E20/1    |     unused, PULL:DOWN |            |              | PR4D  |                                     |
    | E21/1    |     unused, PULL:DOWN |            |              | PR4B  |                                     |
    | E22/1    |     unused, PULL:DOWN |            |              | PR4A  |                                     |
    | F1/5     |     unused, PULL:DOWN |            |              | PL6B  |                                     |
    | F4/5     | led[0]                | LOCATED    | LVCMOS25_OUT | PL5D  |                                     |
    | F5/5     |     unused, PULL:DOWN |            |              | PL3B  | L_GPLLC_FB                          |
    | F6/5     |     unused, PULL:DOWN |            |              | PL2C  |                                     |
    | F7/0     |     unused, PULL:DOWN |            |              | PT9D  |                                     |
    | F8/0     |     unused, PULL:DOWN |            |              | PT11C |                                     |
    | F9/0     |     unused, PULL:DOWN |            |              | PT21C |                                     |
    | F10/0    |     unused, PULL:DOWN |            |              | PT22A |                                     |
    | F11/0    |     unused, PULL:DOWN |            |              | PT23D |                                     |
    | F12/0    |     unused, PULL:DOWN |            |              | PT28B |                                     |
    | F13/0    |     unused, PULL:DOWN |            |              | PT28D |                                     |
    | F14/0    |     unused, PULL:DOWN |            |              | PT31B |                                     |
    | F15/0    |     unused, PULL:DOWN |            |              | PT42C |                                     |
    | F16/0    |     unused, PULL:DOWN |            |              | PT44C | INITN                               |
    | F17/1    |     unused, PULL:DOWN |            |              | PR2C  |                                     |
    | F18/1    |     unused, PULL:DOWN |            |              | PR5C  |                                     |
    | F19/1    |     unused, PULL:DOWN |            |              | PR5D  |                                     |
    | F22/1    |     unused, PULL:DOWN |            |              | PR5A  | DQ0                                 |
    | G1/5     | led[3]                | LOCATED    | LVCMOS25_OUT | PL7B  | PCLKC5_0                            |
    | G2/5     |     unused, PULL:DOWN |            |              | PL7A  | PCLKT5_0                            |
    | G3/5     | led[2]                | LOCATED    | LVCMOS25_OUT | PL6C  |                                     |
    | G4/5     | led[1]                | LOCATED    | LVCMOS25_OUT | PL6D  |                                     |
    | G5/5     |     unused, PULL:DOWN |            |              | PL4C  |                                     |
    | G6/5     |     unused, PULL:DOWN |            |              | PL3C  |                                     |
    | G7/5     |     unused, PULL:DOWN |            |              | PL2D  |                                     |
    | G8/0     |     unused, PULL:DOWN |            |              | PT11D |                                     |
    | G9/0     |     unused, PULL:DOWN |            |              | PT21D |                                     |
    | G11/0    |     unused, PULL:DOWN |            |              | PT23C |                                     |
    | G12/0    |     unused, PULL:DOWN |            |              | PT28A |                                     |
    | G14/0    |     unused, PULL:DOWN |            |              | PT31A |                                     |
    | G15/0    |     unused, PULL:DOWN |            |              | PT42D |                                     |
    | G16/1    |     unused, PULL:DOWN |            |              | PR2D  |                                     |
    | G17/1    |     unused, PULL:DOWN |            |              | PR7C  |                                     |
    | G18/1    |     unused, PULL:DOWN |            |              | PR6D  |                                     |
    | G19/1    |     unused, PULL:DOWN |            |              | PR6C  |                                     |
    | G20/1    |     unused, PULL:DOWN |            |              | PR6B  |                                     |
    | G21/1    |     unused, PULL:DOWN |            |              | PR6A  |                                     |
    | G22/1    |     unused, PULL:DOWN |            |              | PR5B  | DQ0                                 |
    | H1/5     | led[5]                | LOCATED    | LVCMOS25_OUT | PL10B |                                     |
    | H2/5     | led[4]                | LOCATED    | LVCMOS25_OUT | PL10A |                                     |
    | H3/5     |     unused, PULL:DOWN |            |              | PL7D  |                                     |
    | H4/5     |     unused, PULL:DOWN |            |              | PL7C  |                                     |
    | H5/5     |     unused, PULL:DOWN |            |              | PL11A |                                     |
    | H6/5     |     unused, PULL:DOWN |            |              | PL4D  |                                     |
    | H7/5     |     unused, PULL:DOWN |            |              | PL3D  |                                     |
    | H16/1    |     unused, PULL:DOWN |            |              | PR10D |                                     |
    | H17/1    |     unused, PULL:DOWN |            |              | PR10C |                                     |
    | H18/1    |     unused, PULL:DOWN |            |              | PR10B |                                     |
    | H19/1    |     unused, PULL:DOWN |            |              | PR10A |                                     |
    | H20/1    |     unused, PULL:DOWN |            |              | PR7D  |                                     |
    | H21/1    |     unused, PULL:DOWN |            |              | PR7B  | DQ0                                 |
    | H22/1    |     unused, PULL:DOWN |            |              | PR7A  | DQ0                                 |
    | J1/5     | led[7]                | LOCATED    | LVCMOS25_OUT | PL12B |                                     |
    | J2/5     | led[6]                | LOCATED    | LVCMOS25_OUT | PL12A |                                     |
    | J3/5     |     unused, PULL:DOWN |            |              | PL11D |                                     |
    | J4/5     |     unused, PULL:DOWN |            |              | PL11C |                                     |
    | J5/5     |     unused, PULL:DOWN |            |              | PL11B |                                     |
    | J6/5     |     unused, PULL:DOWN |            |              | PL10D |                                     |
    | J7/5     |     unused, PULL:DOWN |            |              | PL10C |                                     |
    | J16/1    |     unused, PULL:DOWN |            |              | PR11A |                                     |
    | J17/1    |     unused, PULL:DOWN |            |              | PR11B |                                     |
    | J18/1    |     unused, PULL:DOWN |            |              | PR11C |                                     |
    | J19/1    |     unused, PULL:DOWN |            |              | PR11D |                                     |
    | J20/1    |     unused, PULL:DOWN |            |              | PR12C |                                     |
    | J21/1    |     unused, PULL:DOWN |            |              | PR12A | DQ0                                 |
    | J22/1    |     unused, PULL:DOWN |            |              | PR12B | DQ0                                 |
    | K1/4     |     unused, PULL:DOWN |            |              | PL14B |                                     |
    | K2/4     |     unused, PULL:DOWN |            |              | PL14A |                                     |
    | K3/4     |     unused, PULL:DOWN |            |              | PL13D |                                     |
    | K4/4     |     unused, PULL:DOWN |            |              | PL13C |                                     |
    | K5/4     |     unused, PULL:DOWN |            |              | PL13B |                                     |
    | K6/5     |     unused, PULL:DOWN |            |              | PL12D |                                     |
    | K7/5     |     unused, PULL:DOWN |            |              | PL12C |                                     |
    | K16/1    |     unused, PULL:DOWN |            |              | PR13D |                                     |
    | K17/1    |     unused, PULL:DOWN |            |              | PR13C |                                     |
    | K18/1    |     unused, PULL:DOWN |            |              | PR13B |                                     |
    | K19/1    |     unused, PULL:DOWN |            |              | PR13A |                                     |
    | K20/1    |     unused, PULL:DOWN |            |              | PR12D |                                     |
    | K22/1    |     unused, PULL:DOWN |            |              | PR16A | DQS0                                |
    | L1/4     |     unused, PULL:DOWN |            |              | PL16A | PCLKT4_0                            |
    | L3/4     |     unused, PULL:DOWN |            |              | PL16C |                                     |
    | L4/4     |     unused, PULL:DOWN |            |              | PL16D |                                     |
    | L5/4     |     unused, PULL:DOWN |            |              | PL14D |                                     |
    | L6/4     |     unused, PULL:DOWN |            |              | PL14C |                                     |
    | L7/4     |     unused, PULL:DOWN |            |              | PL13A |                                     |
    | L16/1    |     unused, PULL:DOWN |            |              | PR14B |                                     |
    | L17/1    |     unused, PULL:DOWN |            |              | PR14A |                                     |
    | L19/1    |     unused, PULL:DOWN |            |              | PR14C |                                     |
    | L20/1    |     unused, PULL:DOWN |            |              | PR14D |                                     |
    | L21/1    |     unused, PULL:DOWN |            |              | PR16B | DQS0N                               |
    | L22/1    |     unused, PULL:DOWN |            |              | PR16C |                                     |
    | M1/4     |     unused, PULL:DOWN |            |              | PL17A |                                     |
    | M2/4     |     unused, PULL:DOWN |            |              | PL16B | PCLKC4_0                            |
    | M5/4     |     unused, PULL:DOWN |            |              | PL17D |                                     |
    | M6/4     |     unused, PULL:DOWN |            |              | PL17C |                                     |
    | M7/4     |     unused, PULL:DOWN |            |              | PL19D |                                     |
    | M16/1    |     unused, PULL:DOWN |            |              | PR18A |                                     |
    | M17/1    |     unused, PULL:DOWN |            |              | PR16D |                                     |
    | M19/1    |     unused, PULL:DOWN |            |              | PR17D |                                     |
    | M20/1    |     unused, PULL:DOWN |            |              | PR17C |                                     |
    | M21/1    |     unused, PULL:DOWN |            |              | PR17B | PCLKC1_0/DQ0                        |
    | M22/1    |     unused, PULL:DOWN |            |              | PR17A | PCLKT1_0/DQ0                        |
    | N1/4     |     unused, PULL:DOWN |            |              | PL17B |                                     |
    | N2/4     |     unused, PULL:DOWN |            |              | PL18A |                                     |
    | N3/4     |     unused, PULL:DOWN |            |              | PL18C |                                     |
    | N4/4     |     unused, PULL:DOWN |            |              | PL18D |                                     |
    | N5/3     |     unused, PULL:DOWN |            |              | PL20B |                                     |
    | N6/3     |     unused, PULL:DOWN |            |              | PL20C |                                     |
    | N7/3     |     unused, PULL:DOWN |            |              | PL20D |                                     |
    | N16/1    |     unused, PULL:DOWN |            |              | PR18B |                                     |
    | N17/1    |     unused, PULL:DOWN |            |              | PR18C |                                     |
    | N18/1    |     unused, PULL:DOWN |            |              | PR18D |                                     |
    | N19/1    |     unused, PULL:DOWN |            |              | PR19D |                                     |
    | N20/1    |     unused, PULL:DOWN |            |              | PR19C |                                     |
    | N22/1    |     unused, PULL:DOWN |            |              | PR19A | DQS1                                |
    | P1/4     |     unused, PULL:DOWN |            |              | PL18B |                                     |
    | P2/4     |     unused, PULL:DOWN |            |              | PL19A |                                     |
    | P3/4     |     unused, PULL:DOWN |            |              | PL19C |                                     |
    | P4/3     |     unused, PULL:DOWN |            |              | PL20A |                                     |
    | P5/3     |     unused, PULL:DOWN |            |              | PL21C |                                     |
    | P6/3     |     unused, PULL:DOWN |            |              | PL21D |                                     |
    | P7/3     |     unused, PULL:DOWN |            |              | PL24D |                                     |
    | P16/1    |     unused, PULL:DOWN |            |              | PR24B |                                     |
    | P17/1    |     unused, PULL:DOWN |            |              | PR24A |                                     |
    | P18/1    |     unused, PULL:DOWN |            |              | PR21D |                                     |
    | P19/1    |     unused, PULL:DOWN |            |              | PR21C |                                     |
    | P20/1    |     unused, PULL:DOWN |            |              | PR20D |                                     |
    | P21/1    |     unused, PULL:DOWN |            |              | PR19B | DQS1N                               |
    | P22/1    |     unused, PULL:DOWN |            |              | PR20C |                                     |
    | PT11A/0  |     unused, PULL:DOWN |            |              | PT11A | L_GPLLT_MFGOUT1                     |
    | PT43A/0  |     unused, PULL:DOWN |            |              | PT43A | R_GPLLT_MFGOUT2                     |
    | R1/4     |     unused, PULL:DOWN |            |              | PL19B |                                     |
    | R2/3     |     unused, PULL:DOWN |            |              | PL21A |                                     |
    | R3/3     |     unused, PULL:DOWN |            |              | PL24A |                                     |
    | R4/3     |     unused, PULL:DOWN |            |              | PL24B |                                     |
    | R5/3     |     unused, PULL:DOWN |            |              | PL24C |                                     |
    | R6/3     |     unused, PULL:DOWN |            |              | PL25C |                                     |
    | R7/3     |     unused, PULL:DOWN |            |              | PL25D |                                     |
    | R16/1    |     unused, PULL:DOWN |            |              | PR26C |                                     |
    | R17/1    |     unused, PULL:DOWN |            |              | PR26B |                                     |
    | R18/1    |     unused, PULL:DOWN |            |              | PR26A |                                     |
    | R19/1    |     unused, PULL:DOWN |            |              | PR25D |                                     |
    | R20/1    |     unused, PULL:DOWN |            |              | PR25C |                                     |
    | R21/1    |     unused, PULL:DOWN |            |              | PR20B | DQ1                                 |
    | R22/1    |     unused, PULL:DOWN |            |              | PR20A | DQ1                                 |
    | T1/3     |     unused, PULL:DOWN |            |              | PL21B |                                     |
    | T2/3     |     unused, PULL:DOWN |            |              | PL25A |                                     |
    | T3/3     |     unused, PULL:DOWN |            |              | PL26A |                                     |
    | T4/3     |     unused, PULL:DOWN |            |              | PL26B |                                     |
    | T5/3     |     unused, PULL:DOWN |            |              | PL26C |                                     |
    | T6/3     |     unused, PULL:DOWN |            |              | PL26D |                                     |
    | T7/3     |     unused, PULL:DOWN |            |              | PL30D |                                     |
    | T8/2     |     unused, PULL:DOWN |            |              | PB8D  |                                     |
    | T9/2     |     unused, PULL:DOWN |            |              | PB16A | MCLK/CCLK                           |
    | T10/2    |     unused, PULL:DOWN |            |              | PB19C |                                     |
    | T11/2    |     unused, PULL:DOWN |            |              | PB22C |                                     |
    | T12/2    |     unused, PULL:DOWN |            |              | PB27B |                                     |
    | T13/2    |     unused, PULL:DOWN |            |              | PB32A |                                     |
    | T14/2    |     unused, PULL:DOWN |            |              | PB32B |                                     |
    | T15/2    |     unused, PULL:DOWN |            |              | PB43C |                                     |
    | T16/2    |     unused, PULL:DOWN |            |              | PB46D |                                     |
    | T17/1    |     unused, PULL:DOWN |            |              | PR27C |                                     |
    | T18/1    |     unused, PULL:DOWN |            |              | PR27B |                                     |
    | T19/1    |     unused, PULL:DOWN |            |              | PR27A |                                     |
    | T20/1    |     unused, PULL:DOWN |            |              | PR26D |                                     |
    | T21/1    |     unused, PULL:DOWN |            |              | PR21B | DQ1                                 |
    | T22/1    |     unused, PULL:DOWN |            |              | PR21A | DQ1                                 |
    | U1/3     |     unused, PULL:DOWN |            |              | PL25B |                                     |
    | U2/3     |     unused, PULL:DOWN |            |              | PL27A | PCLKT3_0                            |
    | U3/3     |     unused, PULL:DOWN |            |              | PL27C |                                     |
    | U4/3     |     unused, PULL:DOWN |            |              | PL27D |                                     |
    | U5/3     |     unused, PULL:DOWN |            |              | PL28D |                                     |
    | U6/2     |     unused, PULL:DOWN |            |              | PB5D  |                                     |
    | U7/2     |     unused, PULL:DOWN |            |              | PB8C  |                                     |
    | U8/2     |     unused, PULL:DOWN |            |              | PB13D |                                     |
    | U9/2     |     unused, PULL:DOWN |            |              | PB16B | SO/SPISO/IO1/MD1/TDIL               |
    | U10/2    |     unused, PULL:DOWN |            |              | PB19D |                                     |
    | U11/2    |     unused, PULL:DOWN |            |              | PB22D |                                     |
    | U12/2    |     unused, PULL:DOWN |            |              | PB27C |                                     |
    | U13/2    |     unused, PULL:DOWN |            |              | PB29D |                                     |
    | U14/2    |     unused, PULL:DOWN |            |              | PB32C |                                     |
    | U15/2    |     unused, PULL:DOWN |            |              | PB38D |                                     |
    | U16/2    |     unused, PULL:DOWN |            |              | PB43D |                                     |
    | U17/1    |     unused, PULL:DOWN |            |              | PR29C |                                     |
    | U18/1    |     unused, PULL:DOWN |            |              | PR28D |                                     |
    | U19/1    |     unused, PULL:DOWN |            |              | PR28C |                                     |
    | U20/1    |     unused, PULL:DOWN |            |              | PR27D |                                     |
    | U21/1    |     unused, PULL:DOWN |            |              | PR24D | DQ1                                 |
    | U22/1    |     unused, PULL:DOWN |            |              | PR24C | DQ1                                 |
    | V1/3     |     unused, PULL:DOWN |            |              | PL27B | PCLKC3_0                            |
    | V4/3     |     unused, PULL:DOWN |            |              | PL28C |                                     |
    | V5/3     |     unused, PULL:DOWN |            |              | PL30C |                                     |
    | V6/2     |     unused, PULL:DOWN |            |              | PB5C  |                                     |
    | V7/2     |     unused, PULL:DOWN |            |              | PB11D |                                     |
    | V8/2     |     unused, PULL:DOWN |            |              | PB13C |                                     |
    | V9/2     |     unused, PULL:DOWN |            |              | PB16C |                                     |
    | V10/2    |     unused, PULL:DOWN |            |              | PB21A |                                     |
    | V11/2    |     unused, PULL:DOWN |            |              | PB24C |                                     |
    | V12/2    |     unused, PULL:DOWN |            |              | PB27D |                                     |
    | V13/2    |     unused, PULL:DOWN |            |              | PB29C |                                     |
    | V14/2    |     unused, PULL:DOWN |            |              | PB32D |                                     |
    | V15/2    |     unused, PULL:DOWN |            |              | PB38C |                                     |
    | V16/2    |     unused, PULL:DOWN |            |              | PB40D |                                     |
    | V17/2    |     unused, PULL:DOWN |            |              | PB46C |                                     |
    | V18/1    |     unused, PULL:DOWN |            |              | PR30A |                                     |
    | V19/1    |     unused, PULL:DOWN |            |              | PR29D |                                     |
    | V22/1    |     unused, PULL:DOWN |            |              | PR25A | DQ1                                 |
    | W1/3     |     unused, PULL:DOWN |            |              | PL28A |                                     |
    | W2/3     |     unused, PULL:DOWN |            |              | PL28B |                                     |
    | W3/3     |     unused, PULL:DOWN |            |              | PL29C |                                     |
    | W4/3     |     unused, PULL:DOWN |            |              | PL30B |                                     |
    | W5/2     |     unused, PULL:DOWN |            |              | PB7D  |                                     |
    | W6/2     |     unused, PULL:DOWN |            |              | PB11C |                                     |
    | W8/2     |     unused, PULL:DOWN |            |              | PB16D |                                     |
    | W9/2     |     unused, PULL:DOWN |            |              | PB18D |                                     |
    | W10/2    |     unused, PULL:DOWN |            |              | PB21B |                                     |
    | W13/2    |     unused, PULL:DOWN |            |              | PB30D |                                     |
    | W14/2    |     unused, PULL:DOWN |            |              | PB33D |                                     |
    | W15/2    |     unused, PULL:DOWN |            |              | PB35D |                                     |
    | W17/2    |     unused, PULL:DOWN |            |              | PB41D |                                     |
    | W18/2    |     unused, PULL:DOWN |            |              | PB44D |                                     |
    | W19/1    |     unused, PULL:DOWN |            |              | PR30C |                                     |
    | W20/1    |     unused, PULL:DOWN |            |              | PR30B |                                     |
    | W21/1    |     unused, PULL:DOWN |            |              | PR28B | DQ1                                 |
    | W22/1    |     unused, PULL:DOWN |            |              | PR25B | DQ1                                 |
    | Y1/3     |     unused, PULL:DOWN |            |              | PL29A |                                     |
    | Y2/3     |     unused, PULL:DOWN |            |              | PL29D |                                     |
    | Y3/3     |     unused, PULL:DOWN |            |              | PL30A |                                     |
    | Y4/2     |     unused, PULL:DOWN |            |              | PB7C  |                                     |
    | Y5/2     |     unused, PULL:DOWN |            |              | PB10C |                                     |
    | Y6/2     |     unused, PULL:DOWN |            |              | PB10D |                                     |
    | Y8/2     |     unused, PULL:DOWN |            |              | PB18C |                                     |
    | Y9/2     |     unused, PULL:DOWN |            |              | PB21C |                                     |
    | Y10/2    |     unused, PULL:DOWN |            |              | PB21D |                                     |
    | Y11/2    |     unused, PULL:DOWN |            |              | PB24D |                                     |
    | Y12/2    |     unused, PULL:DOWN |            |              | PB27A |                                     |
    | Y13/2    |     unused, PULL:DOWN |            |              | PB30C |                                     |
    | Y14/2    |     unused, PULL:DOWN |            |              | PB33C |                                     |
    | Y15/2    |     unused, PULL:DOWN |            |              | PB35C |                                     |
    | Y17/2    |     unused, PULL:DOWN |            |              | PB40C |                                     |
    | Y18/2    |     unused, PULL:DOWN |            |              | PB41C |                                     |
    | Y19/2    |     unused, PULL:DOWN |            |              | PB44C |                                     |
    | Y20/1    |     unused, PULL:DOWN |            |              | PR30D |                                     |
    | Y21/1    |     unused, PULL:DOWN |            |              | PR29B | DQ1                                 |
    | Y22/1    |     unused, PULL:DOWN |            |              | PR28A | DQ1                                 |
    +----------+-----------------------+------------+--------------+-------+-------------------------------------+

    sysCONFIG Pins:
    +----------+--------------------+----------+-------------+
    | Pad Name | sysCONFIG Pin Name | Pin/Bank | Buffer Type |
    +----------+--------------------+----------+-------------+
    | PT15C    | TDO                | E8/0     |             |
    | PT15D    | TDI/MD7            | E9/0     |             |
    | PT22C    | TCK/TEST_CLK       | D10/0    |             |
    | PT22D    | TMS                | C10/0    |             |
    +----------+--------------------+----------+-------------+

    Locate Constraints for each Pin:

    ldc_set_location -site {F4} [ get_ports {led[0]} ]
    ldc_set_location -site {G4} [ get_ports {led[1]} ]
    ldc_set_location -site {G3} [ get_ports {led[2]} ]
    ldc_set_location -site {G1} [ get_ports {led[3]} ]
    ldc_set_location -site {H2} [ get_ports {led[4]} ]
    ldc_set_location -site {H1} [ get_ports {led[5]} ]
    ldc_set_location -site {J2} [ get_ports {led[6]} ]
    ldc_set_location -site {J1} [ get_ports {led[7]} ]
    ldc_set_location -site {D3} [ get_ports {rstn} ]

    Copyright (c) 2002-2024 Lattice Semiconductor Corporation,  All rights reserved.

    Sat Nov 15 12:18:41 2025