@W: CG781 :"C:\Workarea\Projects\LFMXO4-110-EVN\Test_Code\TestCounter_xo4_TestLED\byteCounter.v":44:2:44:9|Input STDBY on instance OSCInst0 is undriven; assigning to 0.  Simulation mismatch possible. Either assign the input or remove the declaration. 
@W: CG133 :"C:\Workarea\Projects\LFMXO4-110-EVN\Test_Code\TestCounter_xo4_TestLED\byteCounter.v":35:12:35:18|Object pllcntr is declared but not assigned. Either assign a value or remove the declaration.
@W: CG360 :"C:\Workarea\Projects\LFMXO4-110-EVN\Test_Code\TestCounter_xo4_TestLED\byteCounter.v":37:7:37:13|Removing wire clk100m, as there is no assignment to it.
@W: CG360 :"C:\Workarea\Projects\LFMXO4-110-EVN\Test_Code\TestCounter_xo4_TestLED\byteCounter.v":38:7:38:14|Removing wire pll_lock, as there is no assignment to it.

