    ###File created by Lattice CPE. Do not modify.###
    create_clock -name {clki_i} -period 10 [get_ports clki_i] originating in instance MyPLL_inst was removed because it is defined at a clock input pin of the IP. User constraints should ensure the corresponding top-level port is correctly constrained at the top-level. If kept it may cause incorrect slack calculation.

    #create_clock -name {clk_p} -period 10 [get_ports clk] originating in top was kept as is.

    # IO_TYPE constraint - Refclk originating in instance MyPLL_inst was updated to # IO_TYPE constraint - Refclk and kept.